# GGSN Charging Gateways

From this dialog box, you can view the charging gateway (CG) details of the GGSN.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN Charging Gateways from the Category drop-down box.

The following information is displayed:

> Gateway Identifier (cgprsCgGatewayIndex)

> Address Type (cgprsCgGatewayAddrType)

> Address (cgprsCgGatewayAddr)

> Gateway Table Row Status (cgprsCgGatewayRowStatus)

> Gateway Status (cgprsCgOperStatus)

> Gateway Reachability (cgprsCgLinkState)

### Gateway Identifier (cgprsCgGatewayIndex)

Unique identifier for the CG.

### Address Type (cgprsCgGatewayAddrType)

Type of Internet address given in cgprsCgGatewayAddr. There are six possible values:

> unknown(0)

> ipv4(1)

> ipv6(2)

> ipv4z(3)

> ipv6z(4)

> dns(16)

### Address (cgprsCgGatewayAddr)

IP address that uniquely identifies the CG.

### Gateway Table Row Status (cgprsCgGatewayRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. cgprsCgGatewayAddrType and cgprsCgGatewayAddr are the mandatory objects in a create request.

- To delete a row, set the object to destroy.

### Gateway Status (cgprsCgOperStatus)

Indicates whether the configured CG is active. There are three possible values:

Value | Description
undefined (1) | Neither in the active nor in the standby mode
active (2) | In the active mode
standby (3) | In the standby mode

### Gateway Reachability (cgprsCgLinkState)

Indicates the status of the CG. There are three possible values:

Value | Description
on | CG is reachable
pending | CG is not reachable but the GGSN is trying to establish a connection with it
off | CG is not reachable