# GGSN Transmitted

From this dialog box, you can view the latest statistics for everything the GGSN has transmitted.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN Transmitted from the Category drop-down box.

The following information is displayed:

> GTP Sent (cGgsnSentSigMessages)

> G-PDU Sent (cGgsnSentGPDUs)

> G-PDU Total Bytes Sent (cGgsnSentGPDUOctets)

> G-PDU Total bytes sent (cGgsnHCSentGPDUOctets)

### GTP Sent (cGgsnSentSigMessages)

Number of GTP signalling messages sent by the GGSN.

### G-PDU Sent (cGgsnSentGPDUs)

Number of G-PDU messages sent by the GGSN.

### G-PDU Total Bytes Sent (cGgsnSentGPDUOctets)

Total number of bytes, sent in G-PDU messages, by the GGSN.

Note: This object is available for versions below GGSN5.0.

### G-PDU Total bytes sent (cGgsnHCSentGPDUOctets)

The number of total bytes sent in G-PDU messages. This counter is updated whenever a G-PDU is sent out by the GGSN.

Note: This object is available for versions above GGSN5.0