# CDMA PDSN Traffic (Octets) Statistics

This dialog box is applicable to Member and Peer to Peer clusters. From here, you can view Code Division Multiple Access (CDMA) service level traffic statistics for octets.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Traffic (Octets) Statistics.

The following data is displayed:

> Simple IP Kilo Octets Transmitted (cCdmaTransmittedSipKiloOctets)

> Simple IP Kilo Octets Received (cCdmaReceivedSipKiloOctets)

> Mobile IP Kilo Octets Transmitted (cCdmaTransmittedMipKiloOctets)

> Mobile IP Kilo Octets Received (cCdmaReceivedMipKiloOctets)

> Proxy Mobile IP Kilo Octets Transmitted (cCdmaTransmittedPmipKiloOctets)

> Proxy Mobile IP Kilo Octets Received (cCdmaReceivedPmipKiloOctets)

> SDB Marked Data Octets (cCdmaTransmittedSDBOctets)

### Simple IP Kilo Octets Transmitted (cCdmaTransmittedSipKiloOctets)

Number of simple IP data octets (in units of 1024 octets) sent to mobile stations from the packet data serving node (PDSN) since system startup.

### Simple IP Kilo Octets Received (cCdmaReceivedSipKiloOctets)

Number of simple IP data octets (in unit of 1024 octets) received from mobile stations since system startup.

### Mobile IP Kilo Octets Transmitted (cCdmaTransmittedMipKiloOctets)

Number of mobile IP data octets (in unit of 1024 octets) sent to mobile stations from the PDSN since system startup.

### Mobile IP Kilo Octets Received (cCdmaReceivedMipKiloOctets)

Number of mobile IP data octets (in unit of 1024 octets) received from mobile stations since system startup.

### Proxy Mobile IP Kilo Octets Transmitted (cCdmaTransmittedPmipKiloOctets)

Number of proxy mobile IP data octets (in unit of 1024 octets) sent to mobile stations since system startup.

### Proxy Mobile IP Kilo Octets Received (cCdmaReceivedPmipKiloOctets)

Number of proxy mobile IP data octets (in unit of 1024 octets) received from mobile stations since system startup.

### SDB Marked Data Octets (cCdmaTransmittedSDBOctets)

Total number of SDB marked data octets sent to PCF from PDSN since system was last restarted.

Note: This object is available for PDSN version 3.0 and later.