# Displaying Chassis Configuration Information

The dialog box displays the chassis configuration information.

## Procedure

> 1. Right-click on the Chassis and select Configure from the pop up menu. The device configuration dialog box appears.

> 2. Select Chassis from the Category drop-down list box.

The following chassis information appears:

> Model (chassisType)

> Chassis ID (chassisId)

> Hardware Version (chassisVersion)

> ROM Monitor Version (romVersion)

> ROM System Version (romSysVersion)

> Processor RAM (processorRam)

> Configuration Memory (bytes) (nvRAMsize)

> Configuration Memory In Use (bytes) (nvRAMUsed)

> Configuration Register (configRegister)

### Model (chassisType)

The type of chassis for the viewed device. For example, c4000 indicates a Cisco 4000 router.

### Chassis ID (chassisId)

Displays the unique number for the chassis. This chassis number contains the value of the CPU serial number or ID number (if available); otherwise, the chassis number is empty. For example, 00160917 is a value for a CPU serial number.

### Hardware Version (chassisVersion)

The chassis hardware revision level, or an empty string if unavailable.

### ROM Monitor Version (romVersion)

The ROM monitor version.

### ROM System Version (romSysVersion)

Displays the software version of the system software in ROM or an empty string if the information is unavailable.

###

### Processor RAM (processorRam)

The amount of RAM, in megabytes, available in the CPU of the device.

### Configuration Memory (bytes) (nvRAMsize)

Displays the amount of nonvolatile configuration memory in bytes.

### Configuration Memory In Use (bytes) (nvRAMUsed)

Specifies the number of bytes of nonvolatile configuration memory in use.

### Configuration Register (configRegister)

The description of the value, in decimal, stored in the configuration register.