# GGSN Access Point

The GGSN Access Point Monitor dialog box lists the IP addresses allocated to MS.

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN Access Point Statistics from the Category list.

3. Select a row and click on Monitor.

4. Select category GGSN Access Point.

The following information appears:

No. of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

Total PDP Context (cgprsAccPtMsActivatedPdps)

Successfully Completed PDP Context (cgprsAccPtSuccMsActivatedPdps)

Dynamic PDP Context (cgprsAccPtMsActivatedDynPdps)

Dynamic PDP Context Completed (cgprsAccPtSuccMsActivatedDynPdps)

PDP Context Deactivation (cgprsAccPtMsDeactivatedPdps)

PDP Context Deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

### No. of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

Number of IP addresses allocated to MS.

### Total PDP Context (cgprsAccPtMsActivatedPdps)

Total number of PDP context activation procedures initiated by any MS on this APN.

### Successfully Completed PDP Context (cgprsAccPtSuccMsActivatedPdps)

Total number of successfully completed PDP context activation procedures initiated by MS on the APN.

### Dynamic PDP Context (cgprsAccPtMsActivatedDynPdps)

Total number of dynamic PDP context activation procedures initiated by the MS on the APN. When an MS requests dynamic PDP address from the PLMN, a dynamic PDP context activation procedure is initiated.

### Dynamic PDP Context Completed (cgprsAccPtSuccMsActivatedDynPdps)

Total number of successfully completed dynamic PDP context activation procedures initiated by MS on the APN.

### PDP Context Deactivation (cgprsAccPtMsDeactivatedPdps)

Total number of PDP context deactivation procedures initiated by the MS on the APN.

### PDP Context Deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

Total number of successfully completed PDP context deactivation procedures initiated by the MS.