# Routed Mode Configuration

The VPN Service Blade Routed Port Mode Setup Wizard dialog box is used to configure the VLAN connection port in the routed mode.

The port routed mode is configured in two steps:

Configure inside interface VLAN

This option lists the existing VLANs configured in the device. You can select one of the existing VLANS, or create a new one by clicking Create.

Configure outside Routed Port

This option configures the VLAN using the name and VLAN ID of the outside interface.

## Procedure

1. Right-click the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard.

2. Click Create. The IPSec VLAN Configuration dialog box appears.

3. Select the radio button Routed Port Mode, then click Configure.... The VPN Service Blade Routed Port Mode Setup Wizard dialog box appears.

The following information appears:

VLAN Interface ID

IP Address

Subnet Mask

Interface Status

Click Create to add a new VLAN.

### VLAN Interface ID

Identifier of the VLAN interface.

### IP Address

IP address assigned to the VLAN.

### Subnet Mask

Subnet mask of the VLAN IP address.

### Interface Status

Status of the VLAN interface.