# SSG TAL User Info Table

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category list.

3. Select a row and click Configure.

4. Select SSG TAL User Info Table from the Category list.

The following information appears:

> User IP Address (cssgTalUserIPAddress)

> User State (cssgTalUserState)

### User IP Address (cssgTalUserIPAddress)

This is the IP address type of a particular transparent user and is used as index (together with cssgTalUserIPAddress) to identify a unique entry in the Tal User Info table.

### User State (cssgTalUserState)

The state of the transparent user.