# Access Point Statistics Monitor1

## Procedure

1. Right-click the device, then select Configure. The Device Configuration dialog box is displayed.

2. Select Access Point Statistics from the Category list.

3. Select the desired row and click Monitor1. The following details are displayed:

> No of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

> Total PDP Context (cgprsAccPtMsActivatedPdps)

> Successfully completed PDP context (cgprsAccPtSuccMsActivatedPdps)

> Dynamic PDP context (cgprsAccPtMsActivatedDynPdps)

> Dynamic PDP context Completed (cgprsAccPtSuccMsActivatedDynPdps)

> PDP context deactivation (cgprsAccPtMsDeactivatedPdps)

> PDP context deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

### No of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

Shows the number of IP addresses allocated to MS.

### Total PDP Context (cgprsAccPtMsActivatedPdps)

The total number of PDP context activation procedures initiated by any MS on this APN.

### Successfully completed PDP context (cgprsAccPtSuccMsActivatedPdps)

The total number of PDP context activation procedures initiated by MS completed successfully.

### Dynamic PDP context (cgprsAccPtMsActivatedDynPdps)

The total number of dynamic PDP context activation procedures initiated by the MS on this APN. When a MS requests dynamic PDP address from the PLMN, a dynamic PDP context activation procedure is initiated.

### Dynamic PDP context Completed (cgprsAccPtSuccMsActivatedDynPdps)

The total number of dynamic PDP context activation procedures initiated by MS completed successfully.

### PDP context deactivation (cgprsAccPtMsDeactivatedPdps)

The total number of PDP context deactivation procedures initiated by the MS on this APN

### PDP context deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

The total number of successfully completed PDP context deactivation procedures initiated by the MS.