# CDMA PDSN Closed RP Registration Statistics - 2

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category list.

3. Select a row and click on Statistics.

4. Select CDMA PDSN Closed RP Registration Statistics from the Category list.

5. Select a row and click on Monitor.

6. Select CDMA PDSN Closed RP Registration Statistics - 2 from the Category list.

The following information appears:

> Incoming-Call-Connected Dropped (ccpcPcfDroppedIccns)

> Call-Disconnect-Notify Received (ccpcPcfRcvdCdns)

> Call-Disconnect-Notify Sent (ccpcPcfSentCdns)

> Call-Disconnect-Notify Dropped (ccpcPcfDroppedCdns)

> Zero-Length-Buffer Recieved (ccpcPcfRcvdZlbs)

> Zero-Length-Buffer Sent (ccpcPcfSentZlb)

### Incoming-Call-Connected Dropped (ccpcPcfDroppedIccns)

Total number of Incoming-Call-Connected messages accepted since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Received (ccpcPcfRcvdCdns)

Total number of Call-Disconnect-Notify messages received to tear down L2TP session since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Sent (ccpcPcfSentCdns)

Total number of Call-Disconnect-Notify messages sent to PCF to tear down L2TP session since the L2TP tunnel was established with PCF.

### Call-Disconnect-Notify Dropped (ccpcPcfDroppedCdns)

Total number of Call-Disconnect-Notify messages dropped since the L2TP tunnel was established with PCF.

### Zero-Length-Buffer Recieved (ccpcPcfRcvdZlbs)

Total number of Zero-Length-Buffer messages received since the L2TP tunnel was established with PCF.

### Zero-Length-Buffer Sent (ccpcPcfSentZlb)

Total number of Zero-Length-Buffer messages sent since the L2TP tunnel was established with PCF.