# SSG Radius Client Table

This dialog box displays details on the Service Selection Gateway (SSG) remote authentication dial-in user service client.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Radius Client Table from the Category list.

The following information is displayed:

> Radius Client Type (cssgRadiusClientAddrType)

> Radius Client Address (cssgRadiusClientAddr)

> Radius Client Rowstatus (cssgRadiusClientRowStatus)

### Radius Client Type (cssgRadiusClientAddrType)

Type of address stored in cssgRadiusClientAddr.

### Radius Client Address (cssgRadiusClientAddr)

Network layer address of the remote authentication dial-in user service (radius) client to which SSG acts as the radius-proxy.

### Radius Client Rowstatus (cssgRadiusClientRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

- To delete a row, set the object to destroy.