# Home Agent Mobile Network Group Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Home Agent Mobile Network Group Configs from the Category list.

The following information appears:

> MR Address Type (cmiHaMrAddrType)

> Inet Address (cmiHaMrAddr)

> MR Dynamic Registration (cmiHaMrDynamic)

> Create/Delete Row (cmiHaMrStatus)

### MR Address Type (cmiHaMrAddrType)

The type of IP address stored in cmiHaMrAddr. Only IPv4 address type is supported.

### Inet Address (cmiHaMrAddr)

The IP address of a mobile router providing mobility to one or more networks. Only IPv4 addresses are supported.

### MR Dynamic Registration (cmiHaMrDynamic)

Specifies whether the mobile router is capable of registering networks dynamically or not.

### Create/Delete Row (cmiHaMrStatus)

The row status for the mobile router entry.