# Foreign Agent Asymmetric Link Support

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Foreign Agent Asymmetric Link Support Configs.

5. Select a row and click the Monitor button.

The following information appears:

> Registration Requests Received for CoA (cmiFaCoaRegAsymLink)

### Registration Requests Received for CoA (cmiFaCoaRegAsymLink)

Number of registration requests that have been received for this care-of address (CoA) on other interfaces (asymmetric links) and have been treated as received on this CoA interface. The count is zero if the CoA interface is not set as transmit-only.