# SRP Error Statistics - History

Use this option to monitor error statistics of an interface side with a specific interval number.

## Procedure

To access SRP error statistics information:

> 1. Right-click the SRP interface and select Configure from the popup menu.

> > The Configure Port dialog box appears.

> 2. Select SRP Error Statistics - History from the Category menu.

> > SRP Error Statistics dialog box displays:

> > Interface Side (srpErrCntIntInterfaceSide)

> > Interface Number (srpErrCntIntNumber)

3. Select an Interval to view error statistics history for that particular interval.

## Related Topics

SRP Physical Layer Errors

SRP Higher Layer Errors

### Interface Side (srpErrCntIntInterfaceSide)

Interface side containing this row information.

### Interface Number (srpErrCntIntNumber)

A number between 1 and 96, which identifies an interval with available statistics.

1 means interval is the most recent completed 15 minute interval.

N means interval precedes N-1.