# CDMA PDSN Cluster Controller Table

This dialog box is applicable to Member clusters. From here, you can view the packet data serving node (PDSN) cluster controller details for this card.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN Cluster Controller Table.

The following information is displayed:

> Controller Address Type (cCdmaClusterCtrlAddressType)

> Controller Address (cCdmaClusterCtrlAddress)

> Controller Status (cCdmaClusterCtrlStatus)

### Controller Address Type (cCdmaClusterCtrlAddressType)

IP address type of a particular controller. The address type, combined with the control address, is used as an index to identify a unique cluster controller entry.

### Controller Address (cCdmaClusterCtrlAddress)

IP address of a particular controller. The controller address, along with the address type, is used as an index to identify a unique cluster controller entry.

### Controller Status (cCdmaClusterCtrlStatus)

Operational status of the cluster controller maintained by the member. There are three possible values:

Value | Description
1 | notConfigured
2 | configured
3 | alive