# Management

Device>Configure>Management

Device management involves displaying and changing information regarding the device itself, for example, information about its physical location and description, information regarding its IP configuration, and device access information.

The CiscoView Configure Device Management window displays the following MIB information:

Device Name (sysName)

Specifies the device domain name. The name can have a maximum of 255 characters.

Contact (sysContact)

Name of the network administration manager and information on how to contact this person. The contact name can contain up to 255 characters.

Location (sysLocation)

Physical location of the device. The location description can have a maximum of 255 characters.

Descriptor (sysDescr)

Textual description of the device.

Up Since (sysUpTime)

Time (in hundredths of a second) since the network management portion of the system was last re-initialized.

Services (sysServices)

Value which indicates the set of services that this device offers.

Click Apply to make your changes take effect, or click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.

RGMP (mcastEnableRgmp)

Indicates whether Router Group Management Protocol is enabled on the device or not. When RGMP is enabled in conjunction with Cisco routers running RGMP, multicast data traffic is forwarded only to those multicast routers that are interested to receive that data traffic. IGMP snooping feature must be enabled on the system to make RGMP feature operational. This object is only supported on platforms that support RGMP feature.

Displayed for the Cat5000, Cat5500, and Cat6000 series devices, version 5.4 or higher.

Click Apply to make your changes take effect, or click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.