# NAM Web Interface

Network Analysis Module (NAM) > Web Interface

For more information on the Network Analysis Module, please refer to the following URL: http://www.cisco.com/warp/public/cc/pd/ifaa/6000nam/prodlit/namca_ov.htm

The following information is displayed:

Protocol

Protocol used to open the Catalyst 6000 NAM Traffic Analyzer application - HTTP or HTTPS.

Note: If the protocol selected in this field is different from the protocol this module is configured for, you will receive an error message after attempting to launch the application.

Port

Port number of the selected protocol. The default value is 80 for HTTP, and 443 for HTTPS.

Note: If the port specified in this field is different from the port configured to accept connections, you will receive an error message after attempting to launch the Catalyst 6000 NAM Traffic Analyzer application.

Click Launch to open the Catalyst 6000 NAM Traffic Analyzer application. Click Cancel to close the dialog box. Click Help to access online help.