Unusual Token Ring Errors

Select Unusual Token Ring Errors from the CATEGORY menu to display the following information in the CiscoView Monitor Port dialog box:

Internal Errors

Frequency Errors

Aborted Trans

Remove Ring Station Requests

Lobe Data Path Errs

Signals Lost

Internal Errors (dot5StatsInternalErrors)

This counter increments each time a station diagnoses an internal error.

Frequency Errors (dot5StatsFreqErrors)

Indicates the number of times that the frequency of the incoming signal is found to be outside the expected range.

Aborted Trans (AbortTransErrors)

This counter increments each time the station transmits an abort delimiter.

Remove Ring Station Reqs (dot5StatsRemove)

Indicates the number of times the interface has detected an open or short circuit in the lobe data path.

Lobe Data Path Errors (dot5StatsLobeErrors)

Shows the number of times the interface has detected an open or short circuit in the lobe data path.

Signals Lost (dot5StatsSignalLoss)

Indicates the number of times the specified interface detected loss of signal.