# PVC Configuration

The PVC Configuration dialog box displays the parameters of the PVC tunnels defined on this port.

VPI (capvcVPI)

VPI value for this PVC.

VCI (capvcVCI)

VCI value for this PVC.

VLAN (capvcVlanId)

Number of the VLAN to which this PVC is bound.

Peak Cell Rate (capvcPCR)

Bandwidth allocation for this PVC, in Kbps.

LoopBack (capvcOAM)

Whether an F5 OAM loopback cell will be sent on this PVC.

Frequency (capvcFrequency)

If the Loopback value is true, this value indicates how often, in seconds, an F5 OAM loopback cell will be sent on this PVC.

Click Set Up PVC to create a new PVC tunnel, or click Modify PVC to edit an existing one.

Click Delete PVC to delete the selected PVC. Note that this will deactivate the VPI/VCI pair assigned to that PVC.