# IPV6 Access Point Statistics 2

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Statistics.
4. Select GGSN Access Point Statistics from the Category drop-down box.
5. With a table entry selected, click Monitor.
6. Select IPV6 Access Point Statistics2 from the Category drop-down box.

The following information appears:

> MS Deactivated PDPs (cgprsAccPtIpv6MsSuccDeactivatedPdps)

> GGSN Deactivation PDPs (cgprsAccPtIpv6GgsnDeactivatedPdps)

> GGSN Deactivated PDPs (cgprsAccPtIpv6GgsnSuccDeactivatedPdps)

> Upstream Traffic (cgprsAccPtIpv6UpstreamTrafficVolume)

> Downstream Traffic (cgprsAccPtIpv6DownstreamTrafficVolume)

> Upstream Packets (cgprsAccPtIpv6UpstreamPacketCount)

> Downstream Packets (cgprsAccPtIpv6DownstreamPacketCount)

### MS Deactivated PDPs (cgprsAccPtIpv6MsSuccDeactivatedPdps)

Total number of successfully completed IPv6 Packet Data Protocol (PDP) context deactivation procedures initiated by any mobile station (MS) on this access point name (APN).

This object is incremented each time a PDP context deletion response message is sent by the gateway GPRS support node (GGSN) to a serving GPRS support node (SGSN).

### GGSN Deactivation PDPs (cgprsAccPtIpv6GgsnDeactivatedPdps)

Total number of IPv6 PDP context deactivation procedures initiated by the GGSN on this APN.

This object is incremented each time a PDP context deletion request message is sent by the GGSN to a SGSN.

### GGSN Deactivated PDPs (cgprsAccPtIpv6GgsnSuccDeactivatedPdps)

Total number of successfully completed IPv6 PDP context deactivation procedures initiated by the GGSN on this APN.

This object is incremented each time a PDP context deletion response message is received by the GGSN from a SGSN.

### Upstream Traffic (cgprsAccPtIpv6UpstreamTrafficVolume)

Total payload volume of upstream traffic processed by this APN. Data flow from an MS to a PDN is considered as upstream traffic.

This object is incremented each time upstream traffic is routed to a PDN.

what does pdn stand for?

### Downstream Traffic (cgprsAccPtIpv6DownstreamTrafficVolume)

Total payload volume of downstream traffic processed by this APN. Data flow from a PDN to an MS is considered as downstream traffic.

This object is incremented each time downstream traffic is routed to a PDN.

### Upstream Packets (cgprsAccPtIpv6UpstreamPacketCount)

Total number of upstream packets sent by this APN. Data flow from an MS to a PDN is considered as upstream traffic.

This object is incremented each time upstream traffic is routed to a PDN.

### Downstream Packets (cgprsAccPtIpv6DownstreamPacketCount)

Total number of downstream packets sent by this APN. Data flow from a PDN to an MS is considered as downstream traffic.

This object is incremented each time downstream traffic is routed to a PDN.