# System Configuration

Device>Configure>Chassis

Host Name (hostName)

This variable represents the name of the host in printable ASCII characters.

System Boot Host Address (sysConfigAddr)

Holds the address of the host that supplied the system boot image.

System Description (sysDescr)

A textual description of the entity. This value should include the full name and version identification of the system's hardware type, software operating-system, and networking software.

ROM Monitor Version (romVersion)

ROM monitor version.

*Firmware Revision (entPhysicalFirmwareRev)

Firmware version of the card being managed (for example, 2.0).

ROM System Version (romSysVersion)

ROM system software version. If version is unavailable, the string will be empty.

*Software Revision (entPhysicalSoftwareRev)

Software version of the card being managed (for example, 3.2).

Configuration Memory (bytes) (nvRAMSize)

Bytes of non-volatile configuration memory.

*Configuration Memory (bytes) (ceExtNVRAMSize)

Total number of bytes of NVRAM in the entity.

Configuration Memory In Use (bytes) (nvRAMUsed)

Bytes of non-volatile configuration memory in use.

*Configuration Memory In Use (bytes) (ceExtNVRAMUsed)

Number of bytes of NVRAM in use.This object is irrelevent if ceExtNVRAMSize is 0.

Configuration Register (configRegister)

Value of configuration register.

*Configuration Register (ceExtConfigRegister)

The value of configuration register with which the processor module booted.

IOS Name (sysConfigName)

Holds the name of the system boot image.

System Boot Protocol (sysConfigProto)

Holds the protocol that supplied the system boot image.

Reason of last Reload (whyReload)

This variable contains a printable octet string which contains the reason why the system was last restarted.

Click Cancel to close this dialog box. Click Print to print the contents of the dialog box.

Note: The items given "*" are applicable for MSFC cards available in SuperVisor modules of Virtual Switch System.