# CDMA PDSN Session Update Statistics

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category CDMA PDSN Session Update Statistics.
5. Select a row and click on Monitor.

The following information appears:

> Session Updates Transmitted (cCdmaRpSessUpdTransmittedReqs)

> Registration Update Accepted (cCdmaRpSessUpdAcceptedReqs)

> Unacknowledged Session Update (cCdmaRpSessUpdNotAckedReqs)

> Initial Session Updates (cCdmaRpSessUpdInitTransmittedReqs)

> Retransmitted Session Updates (cCdmaRpSessUpdReTransmittedReqs)

> Acknowledged Session Updates (cCdmaRpSessUpdReceivedAcks)

> Always On Initial Session Updates (cCdmaRpSessUpdAlwaysON)

> RNPDIT Initial Session Updates (cCdmaRpSessUpdRNPDIT)

### Session Updates Transmitted (cCdmaRpSessUpdTransmittedReqs)

Number of A11 Session Updates transmitted since the system was last restarted.

### Registration Update Accepted (cCdmaRpSessUpdAcceptedReqs)

Number of A11 Session Update Acknowledgements received with the Status field set to zero (indicating that the corresponding Registration Update was accepted) since the system was last restarted.

### Unacknowledged Session Update (cCdmaRpSessUpdNotAckedReqs)

Number of A11 Session Update Updates sent, for which no corresponding A11 Registration Acknowledgements received since the system was last restarted.

### Initial Session Updates (cCdmaRpSessUpdInitTransmittedReqs)

Number of initial A11 Session Updates sent, excluding re-transmitted A11 Registration Updates since the system was last restarted.

### Retransmitted Session Updates (cCdmaRpSessUpdReTransmittedReqs)

Number of re-transmitted A11 Session Updates since the system was last restarted.

### Acknowledged Session Updates (cCdmaRpSessUpdReceivedAcks)

Number of A11 Session Update Acknowledgements received since the system was last restarted.

### Always On Initial Session Updates (cCdmaRpSessUpdAlwaysON)

Number of initial A11 Session Updates sent due to Always On since the system was last restarted. Note that this count does not include any retransmissions.

### RNPDIT Initial Session Updates (cCdmaRpSessUpdRNPDIT)

Number of initial A11 Registration Updates sent due to RNPDIT value downloaded, since the system was last restarted. Note that this count does not include any retransmissions.