# Firewall Service Blade: Create Static Route

You can configure the static, using this third option of the firewall service blade setup wizard, or the Configure Static Route option in the Firewall menu

## Navigation

For the Firewall Service Blade Setup Wizard:

1. Right-click the blade, then select Firewall Service Blade Setup Wizard.

2. Click Next till the Configure Static Route option, in the left pane, is selected. The static route details are displayed in the right pane.

3. Click Create.

For the Firewall menu:

1. Right-click the blade, then select Configure Static Route. The static route details are displayed in the right pane.

2. Click Create.

The following information appears:

Firewall Interface

IP Address

Subnet Mask

Gateway

### Firewall Interface

Name of the firewall interface.

### IP Address

IP address assigned to the VLAN

### Subnet Mask

Subnet mask of the VLAN IP address.

### Gateway

IP gateway for the traffic in a particular VLAN.