# GTP Path Statistics 4

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Configure.
4. Select GGSN GTP Path Table from the Category drop-down box.
5. With a table entry selected, click Monitor.
6. Select GTP Path Statistics4 from the Category drop-down box.

The following information appears:

> Locally Deleted PDPs (cGtpNoSgsnLocalDelPDPs)

> Fallback Deleted PDPs (cGtpVerFallbackLocalDelPDPs)

> Total Collisions (cGtpCreateCollideWithDel)

> Version Changes Occured (cGtpVersionChanges)

> Create Requests (cGtpRetransCreatePDPReqs)

> Create as Update Requests (cGtpCreateAsUpdate)

> IPV6 PDPs Rejected (cGtpIpv6PdpActRejects)

> IPv6 PDPs Created (cGtpIpv6CreatedPDPs)

### Locally Deleted PDPs (cGtpNoSgsnLocalDelPDPs)

Number of Packet Data Protocol (PDP) contexts deleted locally without sending a delete PDP request. If General Packet Radio Service (GPRS) is disabled or the gateway GPRS support node (GGSN) is in standby mode, PDP contexts are deleted locally.

### Fallback Deleted PDPs (cGtpVerFallbackLocalDelPDPs)

Number of PDP contexts deleted locally because of a reversion to a previous GPRS Tunneling Protocol (GTP) version.

This object is incremented each time the GGSN receives a version0 PDP context creation request that exists on a GTP version1 path.

### Total Collisions (cGtpCreateCollideWithDel)

Number of collisions that occurred when a PDP context was locally deleted and then recreated.

### Version Changes Occured (cGtpVersionChanges)

Number of GTP version changes that occurred on a serving GPRS support node (SGSN) path.

This object is incremented each time the GGSN receives a version1 PDP context creation request that exists on a GTP version0 path.

### Create Requests (cGtpRetransCreatePDPReqs)

Number of retransmitted PDP context creation requests received.

This object is incremented each time the GGSN receives a PDP creation request with the same sequence number as the previous PDP creation request.

### Create as Update Requests (cGtpCreateAsUpdate)

Number of PDP context creation requests received that are treated as update requests by the GGSN.

This object is incremented each time the GGSN receives a PDP context creation request for an existing context.

### IPV6 PDPs Rejected (cGtpIpv6PdpActRejects)

Number of IPv6 PDP context activation requests rejected by the GGSN.

### IPv6 PDPs Created (cGtpIpv6CreatedPDPs)

Total number of IPv6 PDP contexts successfully created on a SGSN path. This object includes static, dynamic, and IP PDP contexts.