# BGP4 Policy Accounting

The BGP Policy Accounting dialog box displays the different types of traffic on a particular interface.

## Procedure

For CiscoView versions earlier than 5.2:

1. Right-click the device. Then select Configure, or double-click the device. The Device Configuration dialog box appears.

2. Select Protocols from the Category list.

3. Select BGP4 from the SelectProtocol list and click the Details button. The BGP Configuration dialog box appears.

4. Select BGP Policy Accounting from the Category list.

For CiscoView version 5.2 and later:

1. Right-click the device, then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select BGP4 in the Selectprotocol list. Then click the Details button. The BGP4 Configuration dialog box appears.

   Note: The left frame in the dialog box displays the categories and the right frame displays the category details or a table. If a table is displayed, the variable on which the table is indexed and the key values of the index are listed below the category. Double-click the category to view the table and double-click a key value to view details of a particular row in the table.

   Multiple indexes for a table, if any, are listed below the category in a nested manner. Select a key value to view the rows of the table about that value. Select a key value of the lowest indexing variable to view the details of that particular row.

4. Select BGP Policy Accounting from the left pane.

The following information appears:

Traffic Type (cbpAcctTrafficIndex)

## Related Topics

BGP4 General Information

BGP4 Peer Information

BGP4 Received Paths Attributes

### Traffic Type (cbpAcctTrafficIndex)

Integer with value greater than 0 that uniquely identifies a traffic-type. The traffic-type has no intrinsic meaning. It classifies the traffic coming to an interface into different types. It is up to you to configure the various traffic-types on an interface.