# CDMA PDSN Addressing Schema Statistics

The CDMA PDSN Addressing Schema Statistics category of the Monitor Device dialog box displays the handoff statistics of the packet data servicing node (PDSN).

## Procedure

1. Right-click the device, then select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN Addressing Schema Statistics from the Category list.

The following information appears:

Static IP negotiated by Simple Ip (cCdmaAddressStaticSIPs)

Dynamic IP negotiated by Simple Ip (cCdmaAddressDynamicSIPs)

Static IP negotiated by MOIP (cCdmaAddressStaticMIPs)

Dynamic IP negotiated by MOIP (cCdmaAddressDynamicMIPs)

Static IP negotiated by Proxy MOIP (cCdmaAddressStaticPMIPs)

Dynamic IP negotiated byProxy MOIP (cCdmaAddressDynamicPMIPs)

Static IP negotiated byVPDN (cCdmaAddressStaticVPDNs)

Dynamic IP negotiated byVPDN (cCdmaAddressDynamicVPDNs)

### Static IP negotiated by Simple Ip (cCdmaAddressStaticSIPs)

Total number of simple IP calls that negotiated static IP addresses.

### Dynamic IP negotiated by Simple Ip (cCdmaAddressDynamicSIPs)

Total number of simple IP calls that negotiated dynamic IP addresses.

### Static IP negotiated by MOIP (cCdmaAddressStaticMIPs)

Total number of mobile IP calls that negotiated static IP addresses.

### Dynamic IP negotiated by MOIP (cCdmaAddressDynamicMIPs)

Total number of mobile IP calls that negotiated dynamic IP addresses.

### Static IP negotiated by Proxy MOIP (cCdmaAddressStaticPMIPs)

Total number of proxy mobile IP calls that negotiated static IP addresses.

### Dynamic IP negotiated byProxy MOIP (cCdmaAddressDynamicPMIPs)

Total number of proxy mobile IP calls that negotiated dynamic IP addresses.

### Static IP negotiated byVPDN (cCdmaAddressStaticVPDNs)

Total number of VPDN calls that negotiated static IP addresses.

### Dynamic IP negotiated byVPDN (cCdmaAddressDynamicVPDNs)

Total number of VPDN calls that negotiated dynamic IP addresses.