# CDMA PDSN PCF and Service Option-Based RP Session Update

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category CDMA PDSN PCF and Service Option based RP Session Update.

The following information appears:

> Pcf IP Address (cCdmaPcfSoRpSessUpdIpAddr )

> Packet Data Service Option (cCdmaPcfSoRpSessUpdServiceOption)

### Pcf IP Address (cCdmaPcfSoRpSessUpdIpAddr )

IP address of the (Packet Control Function) PCF that serves the mobile node.

### Packet Data Service Option (cCdmaPcfSoRpSessUpdServiceOption)

A packet data service option specifies a means between the mobile station and radio network to establish and maintain cdma2000 traffic channels for packet data service.