# CDMA PDSN Cluster Member Table

This dialog box is applicable to Controller clusters. From here, you can view the packet data serving node (PDSN) cluster member details.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN Cluster Member Table.

The following information is displayed:

> Cluster Member Address Type (cCdmaClusterMemberAddressType)

> Cluster Member Address (cCdmaClusterMemberAddress)

> Cluster Member Status (cCdmaClusterMemberStatus)

> Cluster Member Load (cCdmaClusterMemberLoad)

### Cluster Member Address Type (cCdmaClusterMemberAddressType)

IP address type of the PDSN cluster member. The address type is combined with the cluster member address and used as an index to identify a unique cluster member entry.

### Cluster Member Address (cCdmaClusterMemberAddress)

IP address of the PDSN cluster member. The address is combined with the cluster member address type and used as an index to identify a unique cluster member entry.

### Cluster Member Status (cCdmaClusterMemberStatus)

Operational status of the PDSN. There are three possible values:

Value | Description
1 | unknown—Cluster controller does not know the member status.
2 | ready—Member is ready to serve call setup request.
3 | adminProhibit—Member does not request for new call setup, but maintains existing calls.

### Cluster Member Load (cCdmaClusterMemberLoad)

PDSN cluster member load, as an aggregate percentage of the maximum load that can be serviced.