# Rate Limit Configuration

Dialog box displays following information:

Data Source (ccarConfigDirection)

Type (ccarConfigType)

Access List Index (ccarConfigAccIdx)

Comitted Access Rate (ccarConfigRate)

Rate Limit (ccarConfigLimit)

Extended Rate Limit (ccarConfigExtLimit)

Conform Action (ccarConfigConformAction)

Exceed Action (ccarConfigExceedAction)

### Data Source(ccarConfigDirection)

The data source for the Rate Limit object.

### Type(ccarConfigType)

The type of traffic rate-limited against.

### Access List Index(ccarConfigAccIdx)

The index to the access list if Rate Limit Type is either quick access or standard access.

### Committed Access Rate(ccarConfigRate)

The committed access rate. This is the sustained rate permitted by the rate limit.

### Rate Limit (ccarConfigLimit)

The rate limit is the amount of traffic, in bytes, in excess of the committed access rate, which will be instantaneously permitted by the rate limit.

### Extended Rate Limit(ccarConfigExtLimit)

The Extended Rate Limit is the amount of traffic, in bytes, in excess of the burst limit, which may be conditionally permitted by the rate limit. The probability that the traffic is not permitted increases as the received burst increases.

### Conform Action(ccarConfigConformAction)

Conform Action is the Action taken when the traffic is within the Rate Limit.

### Exceed Action(ccarConfigExceedAction)

Exceed Action is the Action taken when the traffic exceeds the Rate Limit.