# 802.1x Auth Users

## Navigation

Device > Configure > PAE > 802.1x Auth Users

The following information appears:

> Group Name (cpaeUserGroupName)

> User Name (cpaeUserGroupUserName)

> Address Type (cpaeUserGroupUserAddrType)

> User Address (cpaeUserGroupUserAddr)

> User Interface (cpaeUserGroupUserInterface)

> User VLAN (cpaeUserGroupUserVlan)

### Group Name (cpaeUserGroupName)

The name of the group that a user belongs to.

### User Name (cpaeUserGroupUserName)

The name of a user authenticated on a device's port.

### Address Type (cpaeUserGroupUserAddrType)

Indicates which type of address a user's address is.

### User Address (cpaeUserGroupUserAddr)

The address of the host from which a user logged in.

### User Interface (cpaeUserGroupUserInterface)

The interface index that a user is authenticated on.

### User VLAN (cpaeUserGroupUserVlan)

The VLAN that a user belongs to.