# CDMA PDSN A11 Registration Statistics

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category CDMA PDSN A11 Registration Statistics.
5. Select a row and click on Monitor.

The following information appears:

> Accepted A11 for De-established R-P Conn (cCdmaRpDeRegHandoffAcceptedReqs)

> Initial A11 Registration Req (cCdmaRpInitRegReceivedReqs)

> A11 Re- Registration Req (cCdmaRpReRegReceivedReqs)

> A11 De-Registration Req (cCdmaRpDeRegReceivedReqs)

> Handoff A11 Registration Req (cCdmaRpHandoffRegReceivedReqs)

> Accepted Handoff A11 Registration Req (cCdmaRpHandoffRegAcceptedReqs)

> Airlink Start A11 Registration Reg (cCdmaRpReRegAirlinkStarts)

> Airlink Stop A11 Registration Reg (cCdmaRpReRegAirlinkStops)

> Airlink Stop A11 De-Registration Reg (cCdmaRpDeRegAirlinkStops)

### Accepted A11 for De-established R-P Conn (cCdmaRpDeRegHandoffAcceptedReqs)

Total number of accepted A11 Registration Requests meant for de-establishing the already established R-P connections with the Packet Control Function (PCF) from which the mobile node was handed off since the system was last restarted. The Code field in the corresponding Registration Reply message is set to zero.

### Initial A11 Registration Req (cCdmaRpInitRegReceivedReqs)

Number of Initial A11 Registration requests received since the system was last restarted.

### A11 Re- Registration Req (cCdmaRpReRegReceivedReqs)

Number of A11 Re-Registration requests received since system was last restarted.

### A11 De-Registration Req (cCdmaRpDeRegReceivedReqs)

Number of A11 De-Registration requests received since the system was last restarted.

### Handoff A11 Registration Req (cCdmaRpHandoffRegReceivedReqs)

Number of A11 Handoff Registration requests received since the system was last restarted.

### Accepted Handoff A11 Registration Req (cCdmaRpHandoffRegAcceptedReqs)

Total number of accepted handoff A11 Registration Requests meant for the already existing session, since the system was last restarted.

### Airlink Start A11 Registration Reg (cCdmaRpReRegAirlinkStarts)

Number of A11 Re-Registration requests containing Airlink Start since the system was last restarted.

### Airlink Stop A11 Registration Reg (cCdmaRpReRegAirlinkStops)

Number of A11 Re-Registration requests containing Airlink Stop since the system was last restarted.

### Airlink Stop A11 De-Registration Reg (cCdmaRpDeRegAirlinkStops)

Number of A11 De-Registration requests containing Airlink Stop since the system was last restarted.