# RP Update Statistics

Use this to view Packet Control Function (PCF) and Service Option (SO) based RP Update Statistics.

## Procedure

To access RP Update Statistics information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click on RP Update Statistics.

The following information appears:

> Updates Transmitted (cCdmaPcfSoRpUpdTxdReqs )

> Updates Accepted (cCdmaPcfSoRpUpdAcptdReqs)

> Updates Denied (cCdmaPcfSoRpUpdDeniedReqs)

> Updates Not Acknowledged (cCdmaPcfSoRpUpdNotAckedReqs)

> Initial Updates (cCdmaPcfSoRpUpdInitTxdReqs)

> Retransmitted Updates (cCdmaPcfSoRpUpdReTxdReqs )

### Updates Transmitted (cCdmaPcfSoRpUpdTxdReqs )

Number of A11 registration updates transmitted since system startup.

### Updates Accepted (cCdmaPcfSoRpUpdAcptdReqs)

Since system startup, the number of A11 registration acknowledgements received with the Status field set to zero.

### Updates Denied (cCdmaPcfSoRpUpdDeniedReqs)

Since system startup, the number of A11 registration acknowledgements received with the Status field set to non-zero.

### Updates Not Acknowledged (cCdmaPcfSoRpUpdNotAckedReqs)

Since system startup, the number of A11 registration updates sent when no corresponding acknowledgements were received.

### Initial Updates (cCdmaPcfSoRpUpdInitTxdReqs)

Since system startup, the number of initial A11 registration updates excluding the re-transmitted updates.

### Retransmitted Updates (cCdmaPcfSoRpUpdReTxdReqs )

Number of re-transmitted A11 registration updates since system startup.