# CDMA PDSN Traffic (Pkts) Statistics

This dialog box is applicable to Member and Peer to Peer clusters. From here, you can view Code Division Multiple Access (CDMA) service level traffic statistics for packets.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Traffic (Pkts) Statistics.

The following data is displayed:

> Simple IP Data Pkts Transmitted (cCdmaTransmittedSipPkts)

> Simple IP Data Pkts Received (cCdmaReceivedSipPkts)

> Mobile IP Data Pkts Transmitted (cCdmaTransmittedMipPkts)

> Mobile IP Data Pkts Received (cCdmaReceivedMipPkts)

> Proxy Mobile IP Data Pkts Transmitted (cCdmaTransmittedPmipPkts)

> Proxy Mobile IP Data Pkts Received (cCdmaReceivedPmipPkts)

### Simple IP Data Pkts Transmitted (cCdmaTransmittedSipPkts)

Number of simple IP data packets sent to mobile stations since system startup.

### Simple IP Data Pkts Received (cCdmaReceivedSipPkts)

Number of simple IP data packets received from mobile stations since system startup.

### Mobile IP Data Pkts Transmitted (cCdmaTransmittedMipPkts)

Number of mobile IP data packets sent to mobile stations since system startup.

### Mobile IP Data Pkts Received (cCdmaReceivedMipPkts)

Number of mobile IP data packets received from mobile stations since system startup.

### Proxy Mobile IP Data Pkts Transmitted (cCdmaTransmittedPmipPkts)

Number of proxy mobile IP data packets sent to mobile stations since system startup.

### Proxy Mobile IP Data Pkts Received (cCdmaReceivedPmipPkts)

Number of proxy mobile IP data packets received from mobile stations since system startup.