# PIM Candidate RP Table

Device > Configure > Multicasting > PIM Candidate RP Table

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) Candidate Rendezvous Point (RP) table.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Candidate RP Group Address (pimCandidateRPGroupAddress)

- Candidate RP Group Mask (pimCandidateRPGroupMask)

- Candidate RP Address (pimCandidateRPAddress)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Candidate RP Group Address (pimCandidateRPGroupAddress)

IP multicast group address that, when combined with pimCandidateRPGroupMask, identifies a group prefix the local router will use when advertising itself as a Candidate-RP.

Candidate RP Group Mask (pimCandidateRPGroupMask)

Multicast group address mask that, when combined with pimCandidateRPGroupAddress, identifies a group prefix the local router will use when advertising itself as a Candidate-RP.

Candidate RP Address (pimCandidateRPAddress)

Unicast address of the interface which will be advertised as a Candidate-RP.