# IMA Link Total Statistics

The table displays following information:

Link Violations

Oif Anomalies

Near End Severely Errored Seconds

Far End Severely Errored Seconds

Near End Unavailable Seconds

Far End Unavailable Seconds

Near End Tx Unusable Seconds

Near End Rx Unusable Seconds

Far End Tx Unusable Seconds

Far End Rx Unusable Seconds

Near End Tx Failures

Near end Rx Failures

Far End Tx Failures

Far End Rx Failures

Tx Stuffs Inserted

Rx Stuffs Inserted

Link Violations (imaLinkTotalImaViolations)

Number of erred, invalid, or missing ICP cells during the previous 24 hours, except during SES-IMA or UAS-IMA conditions.

Oif Anomalies (imaLinkTotalOifAnomalies)

Number of OIF anomalies at the near-end in the previous 24-hour interval. Invalid intervals are counted as 0.

Near End Severely Errored Seconds (imaLinkTotalNeSevErroredSecs)

Number of 1-second intervals containing greater than or equal to 30 per cent of the ICP cells counted as IV-IMAs, or one or more link, LIF, or LODS defects in the previous 24 hours.

Far End Severely Errored Seconds (imaLinkTotalFeSevErroredSecs)

Number of 1-second intervals containing one or more RDI-IMA defects in the previous 24 hours, except during UAS-IMA-FE condition.

Near End Unavailable Seconds (imaLinkTotalNeUnavailSecs)

Number of unavailable seconds at near-end in the previous 24 hours. Count begins at the onset of 10 contiguous SES-IMA and ends at the onset of 10 contiguous seconds with no SES-IMA.

Far End Unavailable Seconds (imaLinkTotalFeUnavailSecs)

Number of unavailable seconds at far-end in the previous 24 hours. Count begins at the onset of 10 contiguous SES-IMA-FE and ends at the onset of 10 contiguous seconds with no SES-IMA-FE.

Near End Tx Unusable Seconds (imaLinkTotalNeTxUnusableSecs)

Number of unusable seconds at the near-end Tx LSM in the previous 24 hours.

Near End Rx Unusable Seconds (imaLinkTotalNeRxUnusableSecs)

Number of unusable seconds at the near-end Rx LSM in the previous 24 hours.

Far End Tx Unusable Seconds (imaLinkTotalFeTxUnusableSecs)

Seconds with Tx unusable indication from far-end Tx LSM in the previous 24 hours.

Far End Rx Unusable Seconds (imaLinkTotalFeRxUnusableSecs)

Seconds with Rx unusable indication from the far-end Rx LSM in the previous 24 hour interval.

Near End Tx Failures (imaLinkTotalNeTxNumFailures)

Number of times a near-end transmit failure alarm has been entered on a link in the previous 24 hours.

Near End Rx Failures (imaLinkTotalNeRxNumFailures)

Number of times a near-end receive failure alarm has been entered on a link in the previous 24 hours.

Far End Tx Failures (imaLinkTotalFeTxNumFailures)

Number of times a far-end transmit failure alarm has been entered on a link in the previous 24 hours.

Far End Rx Failures (imaLinkTotalFeRxNumFailures)

Number of times a far-end receive failure alarm has been entered on a link in the previous 24 hours.

Tx Stuffs Inserted (imaLinkTotalTxStuffs)

Number of stuff events inserted in transmit direction in the previous 24 hours.

Rx Stuffs Inserted (imaLinkTotalRxStuffs)

Number of stuff events detected in receive direction in the previous 24 hours.