# SSG Network Group

This dialog box displays the Service Selection Gateway (SSG) network group details.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Network Group from the Category list.

The following information is displayed:

> Network Group Name (cssgNetworkGrpName)

> Network Address Type (cssgNetworkGrpNetIpType)

> Network Address (cssgNetworkGrpNetIpAddr)

> Network Mask Type (cssgNetworkGrpNetMaskType)

> Network Mask (cssgNetworkGrpNetMask)

> Network Group RowStatus (cssgNetworkGrpNetRowStatus)

### Network Group Name (cssgNetworkGrpName)

Name of the network group. A network group, which is a group of networks, is associated with a server group for traffic redirection. Packets to networks in the network group are directed to servers in the server group.

### Network Address Type (cssgNetworkGrpNetIpType)

Value that represents the type of IP address in the object cssgNetworkGrpNetIpAddr.

### Network Address (cssgNetworkGrpNetIpAddr)

IP address of a network in the network group.

### Network Mask Type (cssgNetworkGrpNetMaskType)

Value that represents the type of address stored in cssgNetworkGrpNetMask.

### Network Mask (cssgNetworkGrpNetMask)

Mask to be combined with the destination address before the destination address is compared to the value in cssgNetworkGrpNetIpAddr.

### Network Group RowStatus (cssgNetworkGrpNetRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

- To delete a row, set the object to destroy.