PATH=/ciscoview/Allshare/if/if00000.htm TITLE=Common Interface Information TEXT=Common Interface Information These interface types are common to a wide range of devices. Displaying Port Configuration Information DS1 DS3 SONET Monitoring Port Performance DS1 DS3 SONET
PATH=/ciscoview/Allshare/if/if00001.htm TITLE=Displaying DS1 Port Configuration Information TEXT=Displaying DS1 Port Configuration Information To display configuration information for a DS1 port, double click on the DS1 port. Alternatively right-click on the port and select Configure from the popup menu. The CiscoView configure port window appears. Select one of the following from the CATEGORY pulldown menu: DS1 Configuration DS1 Fractional Interfaces
PATH=/ciscoview/Allshare/if/if00002.htm TITLE=DS1 Configuration Information TEXT=DS1 Configuration Information To display DS1 configuration information, select DS1 Configuration from the CATEGORY pulldown menu. The following information is displayed: DS1 Interface ID (dsx1LineIndex) DS1 Time Elapsed (dsx1TimeElapsed) DS1 Intervals number (dsx1ValidIntervals) DS1 Line Type (dsx1LineType) DS1 Line Coding (dsx1LineCoding) DS1 Send Code Type (dsx1SendCode) DS1 Circuit Identifier (dsx1CircuitIdentifier) DS1 Loopback Configuration (dsx1LoopbackConfig) DS1 Signal Mode (dsx1SignalMode) DS1 Transmit Clock Source (dsx1TransmitClockSource) DS1 Facility Data Link (dsx1Fdl) DS1 Interface Line Status (dsx1LineStatus) DS1 Interface ID (dsx1LineIndex) Displays the ifIndex value for the corresponding interface. DS1 Time Elapsed (seconds) (dsx1TimeElapsed) Displays the number of seconds that have elapsed since the beginning of the current error measurement period. DS1 Intervals Number (dsx1ValidIntervals) Displays the number of previous intervals (up to 96) for which valid data was collected. DS1 Line Type (dsx1LineType) Specifies the type of line. DS1 Line Coding (dsx1LineCoding) Specifies the kind of zero code suppression used on the link. Send Code Type (dsx1SendCode) Specifies the type of data being sent across the D1 interface (for example, normal or looped data, or some type of test pattern). Circuit Identifier (dsx1CircuitIdentifier) Indicates the transmission vendor&#146;s circuit identifier, which is used to facilitate troubleshooting. Loopback Configuration (dsx1LoopbackConfig) Indicates if and how the interface is looped back. Interface Line Status (dsx1LineStatus) Displays a number that indicates loopback, failure, received alarm, and transmitted alarm information. The possible values of the dsx1LineStatus MIB object are: No Alarm Present (dsx1NoAlarm) Near End LOF (dsx1XmtFarEndLOF) NE Sending AIS (dsx1XmtAIS) NE Signal Loss (dsx1LossOfSignal) E1 TS16 AIS (dsx1T16AIS) NE Sending Tx LOMF (dsx1XmtFarEndLOMF) Other Failures (dsx1OtherFailure) Yellow Alarm (dsx1RcvFarEndLOF) FE Sending AIS (dsx1RcvAIS) Red Alarm (dsx1LossOfFrame) NE Looped (dsx1LoopbackState) FE Sending TS 16 LOMF (dsx1RcvFarEndLOMF) NE detects Test Code (dsx1RcvTestCode) Signal Mode (dsx1SignalMode) Specifies the method used for signaling on this channel. Transmit Clock Source (dsx1TransmitClockSource) Indicates the source of transmit clocking. Facility Data Link (dsx1Fdl) Indicates the Facility Data Link protocol supported.
PATH=/ciscoview/Allshare/if/if00012.htm TITLE=if00012 TEXT=The meanings of possible values of the dsx1LineStatus MIB object are: No alarm present Far end sending LOF (Yellow Alarm) 4 Near end sending LOF 8 Far end sending AIS 16 Near end sending AIS 32 Near end LOF (Red Alarm) 64 Near end loss of signal 128 Near end is looped 256 E1 TS16 AIS 512 Far End sending TS16 LOMF 1024 Near End sending TS16 LOMF 2048 Near End detects a test code 4096 Any other line status If the dsx1LoopbackState bit is set, the loopback in effect can be determinedfrom the dsx1LoopbackConfig object.
PATH=/ciscoview/Allshare/if/if00016.htm TITLE=DS1 Fractional Interfaces TEXT=DS1 Fractional Interfaces To display fractional interface information for the DS1 line, select DS1 Fractional Interfaces from the CATEGORY pulldown menu. The table that appears has three columns. DS1 Physical Interface (dsx1FracIndex) DS1 Channel Number (dsx1FracNumber) DS1 Logical Interface (dsx1FracIfIndex) DS1 Channel Number (dsx1FracNumber) The channel number being used. This number identifies a particular fraction ofthe DS1 line.
PATH=/ciscoview/Allshare/if/if00017.htm TITLE=DS1 Physical Interface (dsx1FracIndex) TEXT=DS1 Physical Interface (dsx1FracIndex) The identifier for the physical DS1 interface (the DS1 line), as distinct fromthe logical DS1 interface . This value is the same for every entry in the table.
PATH=/ciscoview/Allshare/if/if00019.htm TITLE=DS1 Logical Interface (dsx1FracIfIndex) TEXT=DS1 Logical Interface (dsx1FracIfIndex) The DS1 logical interface corresponding to a given fraction or channel , as distinct from the physical interface . Zero if no interface is currently using the channel. A single interface mayoccupy more than one time slot. This value can be used with an SNMP get or walk .
PATH=/ciscoview/Allshare/if/if00020.htm TITLE=Displaying DS3 Port Configuration Information TEXT=Displaying DS3 Port Configuration Information To display information for a DS3 port, double click on the port. Alternatively right click on the port and select Configure from the pop up menu. The CiscoView configure port window appears. You can display DS3 configuration information for the port itself, and interface information for each configured line. To display additional information select one of the following from the CATEGORY pulldown menu: DS3 Configuration DS3 Fractional Interfaces
PATH=/ciscoview/Allshare/if/if00021.htm TITLE=DS3 Configuration Information TEXT=DS3 Configuration Information To display DS3 configuration information, select DS3 Configuration from the CATEGORY pulldown menu while a CT3IP card is selected. The following information is displayed: DS3 Interface ID (dsx3LineIndex) DS3 Line Type (dsx3LineType) DS3 Time Elapsed (dsx3TimeElapsed) DS3 Valid Intervals (dsx3ValidIntervals) DS3 Line Coding (dsx3LineCoding) DS3 Send Code (dsx3SendCode) DS3 Circuit Identifer (dsx3CircuitIdentifier) DS3 Loopback Configuration (dsx3LoopbackConfig) DS3 Line Status (dsx3LineStatus) DS3 Interface ID (dsx3LineIndex) Identifies a DS3/E3 Interface on a managed device. If the ifEntry is directly associated only with this DS3/E3 interface, the value is same as ifIndex. If the ifEntry is not directly associated, then number the dsx3LineIndices with an unique identifier greater than the ifNumber. Choose even numbers for inside interfaces and odd numbers for outside interfaces. DS3 Line Type (dsx3LineType) The kind of DS3 C-bit or E3 application that is implementing this interface. (Affects the interpretation of usage and error statistics.) DS3 Time Elapsed (dsx3TimeElapsed) The number of seconds since the beginning of the current error-measurement period for the near end. DS3 Valid Intervals (dsx3ValidIntervals) The number of previous near-end intervals for which valid data was collected. The value is the number of complete 15-minute near-end intervals since the interface came online, up to a maximum of 96 (24 hours). DS3 Line Coding (dsx3LineCoding) The kind of zero code suppression used on this interface. DS3 Send Code (dsx3SendCode) The type of code that the device is sending across the DS3/E3 interface. DS3 Circuit Identifier (dsx3CircuitIdentifier) The transmission vendor's circuit identifier. Used to help with troubleshooting. DS3 Loopback Configuration (dsx3LoopbackConfig) The loopback configuration of the DS3/E3 interface.
PATH=/ciscoview/Allshare/if/if00030.htm TITLE=DS3 Line Status (dsx3LineStatus) TEXT=DS3 Line Status (dsx3LineStatus) The line status of the interface, including loopback state and failure state.The value can represent multiple failures and a loopback simultaneously because it is a bit map represented as a sum.
PATH=/ciscoview/Allshare/if/if00031.htm TITLE=DS3 Transmit Clock Source (dsx3TransmitClockSource) TEXT=DS3 Transmit Clock Source (dsx3TransmitClockSource) The source of transmit clock, derived from the recovered receive clock ofanother DS3 interface.
PATH=/ciscoview/Allshare/if/if00032.htm TITLE=DS3 Fractional Interfaces TEXT=DS3 Fractional Interfaces To display fractional interface information for the DS3 line, select DS3 Fractional Interfaces from the CATEGORY pulldown menu. The table that appears has three columns. DS3 Physical Interface (dsx3FracIndex) DS3 Channel Number (dsx3FracNumber) DS3 Logical Interface (dsx3FracIfIndex) DS3 Channel Number (dsx3FracNumber) The channel number being used. This number identifies a particular fraction ofthe DS3 line.
PATH=/ciscoview/Allshare/if/if00033.htm TITLE=DS3 Physical Interface (dsx3FracIndex) TEXT=DS3 Physical Interface (dsx3FracIndex) The identifier for the physical DS3 interface (the DS3 line), as distinct fromthe logical DS3 interface . This value is the same for every entry in the table.
PATH=/ciscoview/Allshare/if/if00035.htm TITLE=DS3 Logical Interface (dsx3FracIfIndex) TEXT=DS3 Logical Interface (dsx3FracIfIndex) The DS3 logical interface corresponding to a given fraction or channel , as distinct from the physical interface . Zero if no interface is currently using the given channel. A singleinterface may occupy more than one time slot. This value can be used with an SNMP get or walk .
PATH=/ciscoview/Allshare/if/if00036.htm TITLE=SONET Information Configuration  TEXT=SONET Interface Configuration To display SONET interface configuration, select SONET Interface Configuration from the CATEGORY pulldown menu. The following information is displayed: SONET or SDH Signal (sonetMediumType) Elapsed Time (sonetMediumTimeElapsed ) Valid Intervals (sonetMediumValidIntervals ) Line Coding (sonetMediumLineCoding) Line Type (sonetMediumLineType) Circuit Identifier (sonetMediumCircuitIdentifier) SONET or SDH Signal (sonetMediumType) Identifies whether a SONET or SDH signal is used across this interface. The value can be 1 or 2, as follows: SONET SDH Elapsed Time (sonetMediumTimeElapsed) The number of seconds that have elapsed since the beginning of the current error-measurement period (maximum 900 seconds, partial seconds included). Valid Intervals (sonetMediumValidIntervals) The number of previous 15-minute intervals for which valid data has been stored. SONET devices must support at least this specified number of intervals. Minimum 4 (= 1 hour) Default 32 (= 8 hours) Maximum 96 (= 24 hours) The number of complete 15 minute intervals that the device has actually been online is used if it is less than the number specified here. Line Coding (sonetMediumLineCoding) The line coding for this interface. Values depend on whether it is an electrical or optical interface. Electrical interface: 2 B3ZS (sonetMediumB3ZS) CMI (sonetMediumCMI) Optical interface: Non-Return to Zero (sonetMediumNRZ) Return to Zero (sonetMediumRZ The value 1 is for anything else (sonetMediumOther). Line Type (sonetMediumLineType) Specifies the type of line to which this interface is connected. Lines may be optical fiber or electrical: Optical fiber: 2 short range single mode (sonetShortSingleMode) 3 long range single mode (sonetLongSingleMode) 4 Multi-mode (sonetMultiMode) Electrical: 5 Coaxial (sonetCoax) UTP (sonetUTP) The value 1 is for anything else (sonetOther). Circuit Identifier (sonetMediumCircuitIdentifier) The identifier for the circuit, provided by the TELCO transmission vendor. Use this to help with troubleshooting.
PATH=/ciscoview/Allshare/if/if00043.htm TITLE=Monitoring DS1 Lines TEXT=Monitoring DS1 Lines For a DS1 port (supporting T1 lines), the CiscoView monitor port window displays interface level information by default. From the CATEGORY menu, select one of the following types of port statistics to monitor: Serial Statistics DS1 Current Statistics DS1 Total Statistics DS1 Interval Statistics
PATH=/ciscoview/Allshare/if/if00044.htm TITLE=Monitoring DS1 Current Statistics TEXT=Monitoring DS1 Current Statistics The CiscoView Monitor Port window displays the following current statistical information for a DS1 port: Erred Secs (dsx1CurrentESs) Severe Erred Secs (dsx1CurrentSESs) Severe Erred Framing Secs (dsx1CurrentSEFSs) Unavail Erred Secs (dsx1CurrentUASs) Ctroled Slip Secs (dsx1CurrentCSSs) Path Coding Violates (dsx1CurrentPCVs) Line Erred Secs (dsx1CurrentLESs) Bursty Erred Secs (dsx1CurrentBESs) Degraded Mins (dsx1CurrentDMs) Line Code Violates (dsx1CurrentLCVs) Erred Secs (dsx1CurrentESs) Shows the number of seconds during which errors were recorded for a DS1 interface during the current 15-minute interval. Severe Erred Secs (dsx1CurrentSESs) Shows the number of seconds during which severe errors were recorded for a DS1 interface during the current 15-minute interval. Severe Erred Framing Secs (dsx1CurrentSEFSs) Shows the number of seconds during which severe framing errors were recorded for a DS1 interface during the current 15-minute interval. Unavail Erred Secs (dsx1CurrentUASs) Shows the number of seconds during which for the specified DS1 interface was unavailable during the current 15-minute interval. Ctroled Slip Secs (dsx1CurrentCSSs) Shows the number of seconds during which controlled slips were recorded for a DS1 interface during the current 15-minute interval. Path Coding Violates (dsx1CurrentPCVs) Shows the number of path coding violations recorded for a DS1 interface during the current 15-minute interval. Line Erred Secs (dsx1CurrentLESs) Shows the number of seconds during which line errors were recorded for a DS1 interface during the current 15-minute interval. Bursty Erred Secs (dsx1CurrentBESs) Shows the number of seconds during which bursty errors were recorded for a DS1 interface during the current 15-minute interval. Degraded Mins (dsx1CurrentDMs) Shows the number of degraded minutes recorded for a DS1 interface during the current 15-minute interval. Line Code Violates (dsx1CurrentLCVs) Shows the number of line code violations recorded for a DS1 interface duringthe current 15-minute interval.
PATH=/ciscoview/Allshare/if/if00055.htm TITLE=Monitoring DS1 Total Statistics TEXT=Monitoring DS1 Total Statistics The CiscoView Monitor Port window displays the following total statistical information for a DS1 port: Erred Secs (dsx1TotalESs) Severe Erred Secs (dsx1TotalSESs) Severe Erred Framing Secs (dsx1TotalSEFSs) Unavail Erred Secs (dsx1TotalUASs) Ctroled Slip Secs (dsx1TotalCSSs) Path Coding Violates (dsx1TotalPCVs) Line Erred Secs (dsx1TotalLESs) Bursty Erred Secs (dsx1TotalBESs) Degraded Mins (dsx1TotalDMs) Line Code Violates (dsx1TotalLCVs) Erred Secs (dsx1TotalESs) Shows the number of seconds during which errors were recorded for a DS1 interface during the previous 24-hour interval. Severe Erred Secs (dsx1TotalSESs) Shows the number of seconds during which severe errors were recorded for a DS1 interface during the previous 24-hour interval. Severe Erred Framing Secs (dsx1TotalSEFSs) Shows the number of seconds during which severe framing errors were recorded for a DS1 interface during the previous 24-hour interval. Unavail Erred Secs (dsx1TotalUASs) Shows the number of seconds during which the specified DS1 interface was unavailable during the previous 24-hour interval. Ctroled Slip Secs (dsx1TotalCSSs) Shows the number of seconds during which controlled slips were recorded for a DS1 interface during the previous 24-hour interval. Path Coding Violates (dsx1TotalPCVs) Shows the number of path coding violations recorded for a DS1 interface during the previous 24-hour interval. Line Erred Secs (dsx1TotalLESs) Shows the number of seconds during which line errors were recorded for a DS1 interface during the previous 24-hour interval. Bursty Erred Secs (dsx1TotalBESs) Shows the number of seconds during which bursty errors were recorded for a DS1 interface during the previous 24-hour interval. Degraded Mins (dsx1TotalDMs) Shows the number of degraded minutes recorded for a DS1 interface during the previous 24-hour interval. Line Code Violates (dsx1TotalLCVs) Shows the number of line code violations recorded for a DS1 interface duringthe previous 24-hour interval.
PATH=/ciscoview/Allshare/if/if00066.htm TITLE=Monitoring DS1 Interval Statistics TEXT=Monitoring DS1 Interval Statistics With a Monitor window open on a DS1 interface, select DS1 Interval Statistics from the Category pull-down menu. A list box appears displaying index numbers for the 96 previous 15-minute intervals (24 hours). Each index is the line number plus the interval number, separated by a dot. Select the interval that you want to monitor. The following values are displayed: Erred Secs (dsx1IntervalESs) Severe Erred Secs (dsx1IntervalSESs) Severe Erred Framing Secs (dsx1IntervalSEFSs) Unavail Erred Secs (dsx1IntervalUASs) Ctroled Slip Secs (dsx1IntervalCSSs) Path Coding Violates (dsx1IntervalPCVs) Line Erred Secs (dsx1IntervalLESs) Bursty Erred Secs (dsx1IntervalBESs) Degraded Mins (dsx1IntervalDMs) Line Code Violates (dsx1IntervalLCVs) Erred Secs (dsx1IntervalESs) Shows the number of seconds in which errors were recorded for a DS1 interface during the current 15-minute interval. Severe Erred Secs (dsx1IntervalSESs) Shows the number of seconds in which severe errors were recorded for a DS1 interface during the current 15-minute interval. Severe Erred Framing Secs (dsx1IntervalSEFSs) Shows the number of seconds in which severe framing errors were recorded for a DS1 interface during the current 15-minute interval. Unavail Erred Secs (dsx1IntervalUASs) Shows the number of seconds in which the selected DS1 interface was unavailable during the current 15-minute interval. Ctroled Slip Secs (dsx1IntervalCSSs) Shows the number of seconds in which controlled slips were recorded for a DS1 interface during the current 15-minute interval. Path Coding Violates (dsx1IntervalPCVs) Shows the number of path coding violations recorded for a DS1 interface during the current 15-minute interval. Line Erred Secs (dsx1IntervalLESs) Shows the number of seconds in which line errors were recorded for a DS1 interface during the current 15-minute interval. Bursty Erred Secs (dsx1IntervalBESs) Shows the number of seconds in which bursty errors were recorded for a DS1 interface during the current 15-minute interval. Degraded Mins (dsx1IntervalDMs) Shows the number of degraded minutes recorded for a DS1 interface during the current 15-minute interval. Line Code Violates (dsx1IntervalLCVs) Shows the number of line code violations recorded for a DS1 interface duringthe current 15-minute interval.
PATH=/ciscoview/Allshare/if/if00077.htm TITLE=Monitoring DS1 Performance Statistics TEXT=Monitoring DS1 Performance Statistics Select DS1 Performance Statistics from the Monitor pull-down menu to monitor the following information about DS1 bandwidth forthe selected DS1 interface: %Time Available %Available not Degraded %Available not Sev Erred %Available and Error Free
PATH=/ciscoview/Allshare/if/if00078.htm TITLE=%Time Available TEXT=%Time Available The percentage of time that was available on the selected DS1 interface duringthe preceding 24 hours. This is calculated according to the following formula: (86400 - $ dsx1TotalUASs )/100
PATH=/ciscoview/Allshare/if/if00079.htm TITLE=%Available not Degraded TEXT=%Available not Degraded The percent of time that was available on the selected DS1 interface duringthe preceding 24 hours, excluding degraded minutes. This is calculated accordingto the following formula: ((86400 - ($ dsx1TotalUASs +(60*$ dsx1TotalDMs )))/100)
PATH=/ciscoview/Allshare/if/if00080.htm TITLE=%Available not Sev Erred TEXT=%Available not Sev Erred The percent of time that was available on the selected DS1 interface duringthe preceding 24 hours, excluding time with severe errors. This is calculatedaccording to the following formula: (86400 - ($ dsx1TotalUASs +$ dsx1TotalSESs ))/100
PATH=/ciscoview/Allshare/if/if00081.htm TITLE=%Available and Error Free TEXT=%Available and Error Free The percent of time that was available on the selected DS1 interface duringthe preceding 24 hours, excluding degraded minutes. This is calculated accordingto the following formula: (86400 - ($ dsx1TotalUASs +$ dsx1TotalESs ))/100
PATH=/ciscoview/Allshare/if/if00082.htm TITLE=Monitoring DS3 Lines TEXT=Monitoring DS3 Lines For DS3 ports, the CiscoView monitor port window displays interface level information by default. From the CATEGORY menu, select one of the following types of port statistics to monitor: DS3 Current Statistics DS3 Total Statistics DS3 Interval Statistics
PATH=/ciscoview/Allshare/if/if00083.htm TITLE=Monitoring DS3 Current Statistics TEXT=Monitoring DS3 Current Statistics Select DS3 Current Statistics from the Monitor pull-down menu to monitor the following values: P-bit Erred Secs (dsx3CurrentPESs) P-bit Severely Erred Secs (dsx3CurrentPSESs) Severely Erred Framing Secs (dsx3CurrentSEFSs) Unavail Secs (dsx3CurrentUASs) Line Coding Violates (dsx3CurrentLCVs) P-bit Coding Violates (dsx3CurrentPCVs) Line Erred Secs (dsx3CurrentLESs) P-bit Erred Secs (dsx3CurrentPESs) The number of seconds in the current 15-minute interval during which P-bit errors occurred. P-bit Severely Erred Secs (dsx3CurrentPSESs) The number of seconds in the current 15-minute interval during which severe P-bit errors occurred. Severely Erred Framing Secs (dsx3CurrentSEFSs) The number of seconds in the current 15-minute interval during which severe framing errors occurred. Unavail Secs (dsx3CurrentUASs) The number of seconds in the current 15-minute interval during which DS3 service was unavailable. Line Coding Violates (dsx3CurrentLCVs) The number of line coding violations counted in the current 15-minute interval. P-bit Coding Violates (dsx3CurrentPCVs) The number of P-bit coding violations counted in the current 15-minute interval. Line Erred Secs (dsx3CurrentLESs) The number of seconds in the current 15-minute interval during which lineerrors occurred.
PATH=/ciscoview/Allshare/if/if00091.htm TITLE=Monitoring DS3 Total Statistics TEXT=Monitoring DS3 Total Statistics Select DS3 Total Statistics from the Monitor pull-down menu to monitor the following values: P-bit Erred Secs (dsx3TotalPESs) P-bit Severely Erred Secs (dsx3TotalPSESs) Severely Erred Framing Secs (dsx3TotalSEFSs) Unavail Secs (dsx3TotalUASs) Line Coding Violates (dsx3TotalLCVs) P-bit Coding Violates (dsx3TotalPCVs) Line Erred Secs (dsx3TotalLESs) P-bit Erred Secs (dsx3TotalPESs) The number of seconds in the current 15-minute interval during which P-bit errors occurred. P-bit Severely Erred Secs (dsx3TotalPSESs) The number of seconds in the current 15-minute interval during which severe P-bit errors occurred. Severely Erred Framing Secs (dsx3TotalSEFSs) The number of seconds in the current 15-minute interval during which severe framing errors occurred. Unavail Secs (dsx3TotalUASs) The number of seconds in the current 15-minute interval during which DS3 service was unavailable. Line Coding Violates (dsx3TotalLCVs) The number of line coding violations counted in the current 15-minute interval. P-bit Coding Violates (dsx3TotalPCVs) The number of P-bit coding violations counted in the current 15-minute interval. Line Erred Secs (dsx3TotalLESs) The number of seconds in the current 15-minute interval during which lineerrors occurred.
PATH=/ciscoview/Allshare/if/if00099.htm TITLE=Monitoring DS3 Interval Statistics TEXT=Monitoring DS3 Interval Statistics With a Monitor window open on a DS3 interface, select DS3 Interval Statistics from the Category pull-down menu. A list box appears displaying index numbers for the 96 previous 15-minute intervals (24 hours). Each index is the line number plus the interval number, separated by a dot. Select the interval that you want to monitor. The following values are displayed: P-bit Erred Secs (dsx3IntervalPESs) P-bit Severely Erred Secs (dsx3IntervalPSESs) Severely Erred Framing Secs (dsx3IntervalSEFSs) Unavail Secs (dsx3IntervalUASs) Line Coding Violates (dsx3IntervalLCVs) P-bit Coding Violates (dsx3IntervalPCVs) Line Erred Secs (dsx3IntervalLESs) C-bit Coding Violates (dsx3IntervalCCVs) C-bit Erred Secs (dsx3IntervalCESs) C-bit Severely Erred Secs (dsx3IntervalCSESs) P-bit Erred Secs (dsx3IntervalPESs) A count of seconds during which P-bit errors occurred on the selected DS3 interface during the current 15-minute interval. P-bit Severely Erred Secs (dsx3IntervalPSESs) A count of seconds during which severe P-bit errors occurred for the selected DS3 interface during the current 15-minute interval. Severely Erred Framing Secs (dsx3IntervalSEFSs) A count of seconds during which severe framing errors occurred for the selected DS3 interface during the current 15-minute interval. Unavail Secs (dsx3IntervalUASs) A count of seconds during which the selected DS3 interface was not available during the current 15-minute interval. Line Coding Violates (dsx3IntervalLCVs) A count of coding violations for the selected DS3 interface during the current 15-minute interval. P-bit Coding Violates (dsx3IntervalPCVs) A count of P-bit coding violations for the selected DS3 interface during the current 15-minute interval. Line Erred Secs (dsx3IntervalLESs) A count of seconds during which line errors (BPVs or illegal zero sequences) occurred for the selected DS3 interface during the current 15-minute interval. C-bit Coding Violates (dsx3IntervalCCVs) A count of C-bit coding violations for the selected DS3 interface during the current 15-minute interval. C-bit Erred Secs (dsx3IntervalCESs) A count of seconds during which C-bit errors occurred for the selected DS3 interface during the current 15-minute interval. C-bit Severely Erred Secs (dsx3IntervalCSESs) A count of seconds during which severe C-bit errors occurred for the selectedDS3 interface during the current 15-minute interval.
PATH=/ciscoview/Allshare/if/if00110.htm TITLE=Monitoring SONET Lines TEXT=Monitoring SONET Lines For SONET ports, the CiscoView monitor port window displays interface level information by default. From the CATEGORY menu, select one of the following types of port statistics to monitor: SONET Section Current Statistics SONET Section Interval Statistics SONET Line Current Statistics SONET Line Interval Statistics SONET Path Current Statistics SONET Path Interval Statistics
PATH=/ciscoview/Allshare/if/if00111.htm TITLE=Monitoring SONET Section Current Statistics TEXT=Monitoring SONET Section Current Statistics Select SONET Section Current Statistics from the Monitor pull-down menu to monitor SONET section statistics collected for the current 15 minute interval. The following values are displayed: Erred Secs (sonetSectionCurrentESs) Severely Erred Secs (sonetSectionCurrentSESs) Severely Erred Framing Secs (sonetSectionCurrentSEFSs) Coding Violates (sonetSectionCurrentCVs) Erred Secs (sonetSectionCurrentESs) The number of seconds in the current 15-minute interval in which a SONET/SDH section encountered an error. Severely Erred Secs (sonetSectionCurrentSESs) The number of seconds in the current 15-minute interval in which a SONET/SDH section encountered a severe error. Severely Erred Framing Secs (sonetSectionCurrentSEFSs) The number of seconds in the current 15-minute interval in which a SONET/SDH section encountered a severe framing error. Coding Violates (sonetSectionCurrentCVs) The number of SONET/SDH coding violations in the current 15-minute interval.
PATH=/ciscoview/Allshare/if/if00116.htm TITLE=Monitoring SONET Section Interval Statistics TEXT=Monitoring SONET Section Interval Statistics Select SONET Section from the Category pull-down menu. Select a row from the dialog and click the OK button. The Section Interval Statistics dialog box is displayed with the following details: Errored Seconds (sonetSectionIntervalESs) Severely Errored Seconds (sonetSectionIntervalSESs) Severely Errored Framing Seconds (sonetSectionIntervalSEFSs) Coding Violation (sonetSectionIntervalCVs) Errored Seconds (sonetSectionIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered an error. Severely Errored Seconds (sonetSectionIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered a severe error. Severely Errored Framing Seconds (sonetSectionIntervalSEFSs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered a severe framing error. Coding Violation (sonetSectionIntervalCVs) The number of SONET/SDH coding violations in one of the preceding valid intervals (sonetMediumValidIntervals) .
PATH=/ciscoview/Allshare/if/if00117.htm TITLE=Erred Secs (sonetSectionIntervalESs) TEXT=Erred Secs (sonetSectionIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered an error.
PATH=/ciscoview/Allshare/if/if00118.htm TITLE=Severely Erred Secs (sonetSectionIntervalSESs) TEXT=Severely Erred Secs (sonetSectionIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered a severe error.
PATH=/ciscoview/Allshare/if/if00119.htm TITLE=Severely Erred Framing Secs (sonetSectionIntervalSEFSs) TEXT=Severely Erred Framing Secs (sonetSectionIntervalSEFSs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) in which a SONET/SDH section encountered a severe framing error.
PATH=/ciscoview/Allshare/if/if00120.htm TITLE=Coding Violates (sonetSectionIntervalCVs) TEXT=Coding Violates (sonetSectionIntervalCVs) The number of SONET/SDH coding violations in one of the preceding valid intervals (sonetMediumValidIntervals) .
PATH=/ciscoview/Allshare/if/if00121.htm TITLE=Monitoring SONET Line Current Statistics TEXT=Monitoring SONET Line Current Statistics Select SONET Line Current Statistics from the Monitor pull-down menu to monitor SONET line statistics collected for the current 15 minute interval. The following values are displayed: Erred Secs (sonetLineCurrentESs) Severely Erred Secs (sonetLineCurrentSESs) Coding Violates (sonetLineCurrentCVs) Unavail Secs (sonetLineCurrentUASs) Erred Secs (sonetLineCurrentESs) The number of seconds during the current 15 minute interval that a line error occurred. Severely Erred Secs (sonetLineCurrentSESs) The number of seconds during the current 15 minute interval that a severe error occurred for this line. Coding Violates (sonetLineCurrentCVs) The number of seconds during the current 15 minute interval that a coding violation occurred for this line. Unavail Secs (sonetLineCurrentUASs) The number of seconds during the current 15 minute interval that the line wasnot available.
PATH=/ciscoview/Allshare/if/if00126.htm TITLE=Monitoring SONET Line Interval Statistics TEXT=Monitoring SONET Line Interval Statistics Select SONET Line from the Category pull-down menu. Select a row from the dialog and click the OK button. The Line Interval Statistics dialog box is displayed with the following details: Errored Seconds (sonetLineIntervalESs) Severely Errored Seconds (sonetLineIntervalSESs) Unavailable Seconds (sonetLineIntervalUASs) Coding Violation (sonetLineIntervalCVs) Errored Seconds (sonetLineIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a line error occurred. Severely Errored Seconds (sonetLineIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a severe error occurred for this line. Coding Violation (sonetLineIntervalCVs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a coding violation occurred for this line. Unavailable Seconds (sonetLineIntervalUASs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that the line was not available.
PATH=/ciscoview/Allshare/if/if00127.htm TITLE=Erred Secs (sonetLineIntervalESs) TEXT=Erred Secs (sonetLineIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a line error occurred.
PATH=/ciscoview/Allshare/if/if00128.htm TITLE=Severely Erred Secs (sonetLineIntervalSESs) TEXT=Severely Erred Secs (sonetLineIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a severe error occurred for this line.
PATH=/ciscoview/Allshare/if/if00129.htm TITLE=Coding Violates (sonetLineIntervalCVs) TEXT=Coding Violates (sonetLineIntervalCVs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a coding violation occurred for this line.
PATH=/ciscoview/Allshare/if/if00130.htm TITLE=Unavail Secs (sonetLineIntervalUASs) TEXT=Unavail Secs (sonetLineIntervalUASs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that the line was not available.
PATH=/ciscoview/Allshare/if/if00131.htm TITLE=Monitoring SONET Path Current Statistics TEXT=Monitoring SONET Path Current Statistics Select SONET Path Current Statistics from the Monitor pull-down menu to monitor SONET path statistics collected for the current 15 minute interval. The following values are displayed: Errored Seconds (sonetPathIntervalESs) Severely Errored Seconds (sonetPathIntervalSESs) Unavailable Seconds (sonetPathIntervalUASs) Coding Violation (sonetPathIntervalCVs) Errored Seconds (sonetPathIntervalESs) The number of seconds during the current 15 minute interval that a path error occurred for this path. Severely Errored Seconds (sonetPathIntervalSESs) The number of seconds during the current 15 minute interval that a severe path error occurred for this path. Coding Violates (sonetPathIntervalCVs) The number of seconds during the current 15 minute interval that a coding violation occurred for this path. Unavailable Seconds (sonetPathIntervalUASs) The number of seconds during the current 15 minute interval that the path was not available.
PATH=/ciscoview/Allshare/if/if00136.htm TITLE=Monitoring SONET Path Interval Statistics TEXT=Monitoring SONET Path Interval Statistics Select SONET Path from the Category pull-down menu. Select a row from the dialog and click the OK button. The Path Interval Statistics dialog box is displayed with the following details: Errored Seconds (sonetPathIntervalESs) Severely Errored Seconds (sonetPathIntervalSESs) Unavailable Seconds (sonetPathIntervalUASs) Coding Violation (sonetPathIntervalCVs) Errored Seconds (sonetPathIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a path error occurred. Severely Errored Seconds (sonetPathIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a severe error occurred for this path. Coding Violation (sonetPathIntervalCVs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a coding violation occurred for this path. Unavailable Seconds (sonetPathIntervalUASs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that the path was not available.
PATH=/ciscoview/Allshare/if/if00137.htm TITLE=Erred Secs (sonetPathIntervalESs) TEXT=Erred Secs (sonetPathIntervalESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a line error occurred.
PATH=/ciscoview/Allshare/if/if00138.htm TITLE=Severely Erred Secs (sonetPathIntervalSESs) TEXT=Severely Erred Secs (sonetPathIntervalSESs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a severe error occurred for this line.
PATH=/ciscoview/Allshare/if/if00139.htm TITLE=Coding Violates (sonetPathIntervalCVs) TEXT=Coding Violates (sonetPathIntervalCVs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that a coding violation occurred for this line.
PATH=/ciscoview/Allshare/if/if00140.htm TITLE=Unavail Secs (sonetPathIntervalUASs) TEXT=Unavail Secs (sonetPathIntervalUASs) The number of seconds in one of the preceding valid intervals (sonetMediumValidIntervals) that the line was not available.
PATH=/ciscoview/Allshare/if/if00142.htm TITLE=Displaying Connector Type Information TEXT=Displaying Connector Type Information Interface connector type currently enabled. Valid values for this GBIC moduleare gbic-sx, gbic-lx, gbic-lh, gbic-cx, gbic-missing.
PATH=/ciscoview/Allshare/if/if00143.htm TITLE=Rate Limit Status TEXT=Rate Limit Status The Rate Limit Status dialog box displays the following information: Packets Permitted (ccarStatSwitchedPkts) Bytes Permitted (ccarStatSwitchedBytes) Packets Exceeding Limit (ccarStatFilteredPkts) Bytes Exceeding Limit (ccarStatFilteredBytes) Burst Size (ccarStatCurBurst) Packets Permitted(ccarStatSwitchedPkts) The counter of packets permitted by the rate limit. Bytes Permitted(ccarStatSwitchedBytes) The counter of bytes permitted by the interface. Packets Exceeding Limit(ccarStatFilteredPkts) The counter of packets which exceeded the rate limit. Bytes Exceeding Limit(ccarStatFilteredBytes) The counter of bytes, which exceeded the rate limit. Burst Size(ccarStatCurBurst) The current received burst size.
PATH=/ciscoview/Allshare/if/if00149.htm TITLE=Monitoring IP Precedence Statistics TEXT=Monitoring IP Precedence Statistics The IP Precedence Statistics dialog box displays the following information: Traffic in Packets (cipPrecedenceSwitchedPkts) Traffic in Bytes (cipPrecedenceSwitchedBytes) Traffic in Packets(cipPrecedenceSwitchedPkts) Traffic, in Packets, at the cipPrecedecndeIpPrecedence Precedence. Traffic in Bytes(cipPrecedenceSwitchedBytes) Traffic, in Bytes, at the cipPrecedenceIpPrecedence precedence.
PATH=/ciscoview/Allshare/if/if00152.htm TITLE=Monitoring IP MAC Statistics TEXT=Monitoring IP MAC Statistics The IP MAC Statistics dialog box provides the following information: Traffic in Packets (cipMacSwitchedPkts) Traffic in Bytes (cipMacSwitchedBytes) Traffic in Packets(cipMacSwitchedPkts) Traffic in Packets indicates the counter in packets with respect to cipMacAddress. Traffic in Bytes(cipMacSwitchedBytes) Traffic in bytes gives the counter in bytes with respect to the cipMacAddress.
