# IMA Link Configuration Table

The table displays the following information:

> Interface Index

> Row Status

> Group Index

> Near End Transmission State

> Near End Reception State

> Far End Transmission State

> Far End Reception State

> Near End Rx Failure Status

> Far End Rx Failure status

> Transmission Id

> Reception Id

> Relative Delay

> Test Status

> Time Elapsed

### Interface Index (imaLinkIfIndex)

Indicates the logical number assigned to an IMA link.

### RowStatus (imaLinkRowStatus)

Indicates the status of a row in the table.

### Group Index (imaLinkGroupIndex)

Indicates the IMA group (imaGroupIndex) of which this link is a member.

### Near End Transmission State (imaLinkNeTxState)

Indicates the state of the near-end transmit link.

### Near End Reception State (imaLinkNeRxState)

Indicates the state of the near-end receive link.

### Far End Transmission State (imaLinkFeTxState)

Indicates the state of the far-end transmit link as reported through ICP cells.

### Far End Reception State (imaLinkFeRxState)

Indicates the state of the far-end receive link as reported through ICP cells.

### Near End Rx Failure status (imaLinkNeRxFailureStatus)

Indicates the current link failure status of the near-end receive link.

### Far End Rx Failure status (imaLinkFeRxFailureStatus)

Indicates the link failure status of the far-end receive link as reported through ICP cells.

### Transmission Id (imaLinkTxLid)

Indicates the outgoing link ID used by the local end. The transmission ID is valid only when the link belongs to an IMA group.

### Reception Id (imaLinkRxLid)

Indicates the incoming link ID used by the remote end as reported via ICP cells. The reception ID is valid only when the link belongs to an IMA group.

### Relative Delay (imaLinkRelDelay)

Indicates the latest measured delay on a link relative to the link with the least delay. For the relative delay to be valid, both the links should be in the same IMA group.

### Test status (imaLinkTestProcStatus)

Indicates the state of the test pattern procedure.

Value | Description
Disabled (1) | The test is not running.
Operating (2) | The test is running and no error has been found on the interface.
LinkFail (3) | An error has been detected on a link during the test.

After an error occurs, the link fail value is latched, until the object is read or the imaGroupTestProcStatus is moved to disabled. After the error is read, and if it longer persists, a subsequent read will reports the value Operating.

### Time Elasped (imaLinkTimeElapsed)

Indicates the time elapsed since the beginning of the measurement period in seconds.