# CDMA PDSN Registration Failures (contd..)

Use this option to view rejected registration statistics.

## Procedure

To access CDMA PDSN registration failure information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Registration Failures (contd..) from the Category menu.

Registration Failures dialog box displays:

Registration Request Failed Unknown PDSN/HA (cCdmaRpRegUnknownPdsnFailures)

Registration Request Failed Reverse Tunnel (cCdmaRPRegNoRevTunnelFailures)

Registration Request Failed T bit (cCdmaRPRegTBitNotSetFailures)

Registration Request Failed CVSE (cCdmaRPRegBadCVSEFailures)

### Registration Request Failed Unknown PDSN/HA (cCdmaRpRegUnknownPdsnFailures)

Number of registration requests failed due to unknown HA (Home Agent) address since system startup.

### Registration Request Failed Reverse Tunnel (cCdmaRPRegNoRevTunnelFailures)

Number of registration requests failed due to FA (Foreign Agent) to HA tunnel setup failure since system startup.

### Registration Request Failed T bit (cCdmaRPRegTBitNotSetFailures)

Number of registration requests failed due to unset T bit since system startup.

### Registration Request Failed CVSE (cCdmaRPRegBadCVSEFailures)

Number of registration requests failed due to unsupported vendor code in CVSE since system startup.