# IPv6 GGSN Statistics

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Statistics.
4. Select IPv6 GGSN Statistics from the Category drop-down box.

The following information appears:

> Successfully Created (cGgsnTotalCreatedIPv6Pdps)

> Deleted PDPs (cGgsnTotalDeletedIPv6Pdps)

> Rejected PDPs (cGgsnTotalRejectedIPv6Pdps)

> Messages Sent (cGgsnSentIPv6SigMessages)

> Messages Received (cGgsnReceivedIPv6SigMessages)

> Packets Sent (cGgsnSentIPv6PDUs)

> Packets Received (cGgsnReceivedIPv6PDUs)

> PDUs Sent (cGgsnSentIPv6PDUOctets)

> PDUs Received (cGgsnReceivedIPv6PDUOctets)

### Successfully Created (cGgsnTotalCreatedIPv6Pdps)

Total number of successfully created IPv6 Packet Data Protocol (PDP) contexts.

This object is incremented each time an IPv6 PDP context is created. This includes static, dynamic, and IP PDP contexts.

### Deleted PDPs (cGgsnTotalDeletedIPv6Pdps)

Total number of IPv6 PDP contexts deleted.

This object is incremented each time an IPv6 PDP context is deleted. This includes static, dynamic, IP, and Point-to-Point Protocol (PPP) PDP contexts.

### Rejected PDPs (cGgsnTotalRejectedIPv6Pdps)

Total number of rejected IPv6 PDP context activation requests.

This object is incremented each time an IPv6 PDP context activation request is rejected.

### Messages Sent (cGgsnSentIPv6SigMessages)

Total number of GPRS Tunneling Protocol (GTP) signaling messages related to IPv6 PDP contexts sent by the gateway GPRS support node (GGSN).

This object is incremented each time a GTP signaling message for IPv6 PDP contexts is sent out (including retries).

### Messages Received (cGgsnReceivedIPv6SigMessages)

Total number of GTP signaling messages related to IPv6 PDP contexts received by the GGSN.

This object is incremented each time a GTP signaling message for IPv6 PDP contexts is received.

### Packets Sent (cGgsnSentIPv6PDUs)

Number of IPv6 data packets sent by the GGSN.

This object is incremented each time a G-PDU is sent out.

g-pdu message?

### Packets Received (cGgsnReceivedIPv6PDUs)

Number of IPv6 data packets received by the GGSN.

This object is incremented each time a G-PDU is received.

### PDUs Sent (cGgsnSentIPv6PDUOctets)

Number of IPv6 data bytes sent in PDU messages by the GGSN.

This object is incremented each time a G-PDU is sent out.

### PDUs Received (cGgsnReceivedIPv6PDUOctets)

Number of IPv6 data bytes received in PDU messages by the GGSN.

This object is incremented each time a G-PDU is received.