# OSPF Stub Area Configuration

The OSPF Stub Area Configuration dialog box displays the stub area configuration details for OSPF.

## Procedure

For CiscoView versions earlier than 5.2:

1. Right-click the device. Then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list. Then click the Details button. The OSPF Configuration dialog box appears.

4. Select Stub Area Configuration from the Category list.

For CiscoView version 5.2 and later:

1. Right-click the device, then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list, then click the Details button. The OSPF Configuration dialog box appears.

   Note: The left frame in the dialog box displays the categories and the right frame displays the category details or a table. If a table is displayed, the variable on which the table is indexed and the key values of the index are listed below the category. Double-click the category to view the table and double-click a key value to view details of a particular row in the table.

   Multiple indexes for a table, if any, are listed below the category in a nested manner. Select a key value to view the rows of the table about that value. Select a key value of the lowest indexing variable to view the details of that particular row.

4. Select Stub Area Configuration from the left pane.

The following information appears:

Stub Area ID (ospfStubAreaID)

Type of Service (ospfStubTOS)

Metric Value (ospfStubMetric)

Metric Entry Validity (ospfStubStatus)

## Related Topics

OSPF Address Range Configuration

OSPF Area Configuration

OSPF General Configuration

OSPF Host Configuration

OSPF Interface Configuration

OSPF Link State Database

OSPF Neighbor Configuration

OSPF ToS Metrics for Nonvirtual Interface

OSPF Virtual Neighbor Configuration

OSPF Virtual Interface Configuration

### Stub Area ID (ospfStubAreaID)

32 bit identifier for the stub area. On creation, this can be derived from the instance.

### Type of Service (ospfStubTOS)

Type of service associated with the metric. On creation, this can be derived from the instance.

### Metric Value (ospfStubMetric)

Metric value applied at the indicated type of service. By default, this equals the least value at the type of service among the interfaces to other areas.

### Metric Entry Validity (ospfStubStatus)

Indicates the validity or invalidity of the entry. Setting it to invalid has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent.