# Host Configurations

## Navigation

Device > Configure > EOU > Host Configurations

The following information appears:

> Host Validation (cnnEouHostValidateAction)

> IP Addr Type (cnnEouHostValidateIpAddrType)

> IP Address (cnnEouHostValidateIpAddr)

> MAC Address (cnnEouHostValidateMacAddr)

> Posture Token Type (cnnEouHostValidatePostureToken)

> Max Query Entries (cnnEouHostMaxQueries)

> Validate Posture Token String (cnnEouHostValidatePostureTokenStr)

### Host Validation (cnnEouHostValidateAction)

EOU validation setting configured for the devices associated with the system.

When a device is initialized, all previous state information for that device is deleted and the admission control process starts with no active state. When a device is revalidated, state information for that device is retained so that the device still has its normal access privileges during the revalidation process.

There are 15 possible values:

> none(1): No operation is performed.

> initializeAll(2): Manually initiates reauthentication of all endpoint devices on the system.

> initializeAuthClientless(3): Manually initiates reauthentication of all clientless endpoint devices.

> initializeAuthEap(4): Manually initiates reauthentication of all endpoint devices authorized by the Extensive Authentication Protocol (EAP).

> initializeAuthStatic(5): Manually initiates reauthentication of all statically authorized endpoint devices.

> initializeIp(6): Manually initiates reauthentication of a specific IP device. The values of cnnEouHostValidateIpAddrType and cnnEouHostValidateIpAddr are used by this operation.
> initializeMac(7): Manually initiates reauthentication of the endpoint device, identified by its MAC address. The value of cnnEouHostValidateMacAddr is used by this operation.

> initializePostureToken(8): Manually initiates reauthentication of the endpoint devices with a specific posture token assigned. The value of cnnEouHostValidatePostureToken is used by this operation.

> revalidateAll(9): Revalidates the EOU posture credentials of all devices on the system.

> revalidateAuthClientless(10): Revalidates the EOU posture credentials of all clientless devices on the system.

> revalidateAuthEap(11): Revalidates the EOU posture credentials of the devices authorized by EAP on the system.

> revalidateAuthStatic(12): Revalidates the EOU posture credentials of all statically authorized devices on the system.

> revalidateIp(13): Revalidates the EOU posture credentials of a specific device, identified by its IP address. The values of cnnEouHostValidateIpAddrType and cnnEouHostValidateIpAddr are used by this operation.

> revalidateMac(14): Revalidates the EOU posture credentials of a specific device, identified by its MAC address. The value of cnnEouHostValidateMacAddr is used by this operation.

> revalidatePostureToken(15): Revalidates the EOU posture credentials of devices with the specific posture token assigned. The value of cnnEouHostValidatePostureToken is used by this operation.

Note: This object always returns the value none when read.

### IP Addr Type (cnnEouHostValidateIpAddrType)

IP address type for a detected host.

### IP Address (cnnEouHostValidateIpAddr)

IP address of a detected host. The address type is determined by the value of cnnEouHostValidateIpAddrType.

### MAC Address (cnnEouHostValidateMacAddr)

MAC address of a detected host.

### Posture Token Type (cnnEouHostValidatePostureToken)

Type of posture token.

### Max Query Entries (cnnEouHostMaxQueries)

Maximum number of query entries allowed to be outstanding at any time in cnnEouHostQueryTable.

### Validate Posture Token String (cnnEouHostValidatePostureTokenStr)

Posture token string for a detected host.