# X.25 Operational Status

The CiscoView Configure window displays the following operational status information for a port configured for X.25:

Interface Mode

Max Supported Circuits

No PVCs Configured

Data Link ID

X.25 Protocol Version

# Interface Mode (linfConf)

Displays the line card type.

# Max Supported Circuits (x25AdmnMaxActiveCircuits)

Specifies the maximum number of concurrent circuits (including PVCs) that can be supported at this interface.

# No PVCs Configured (x25AdmnNumberPVCs)

Specifies the number of Permanent Virtual Circuits (PVCs) configured for this interface. The PVCs use channel numbers from this number.

# Data Link ID (x25OperDataLinkId)

Displays the object identifier of the supporting layer 2 interface.

# X.25 Protocol Version (x25AdmnProtocolVersionSupported)

Displays an object identifier that refers to a specific version of the X.25 packet layer protocol.