# Configure Outside Routed Port

The Configure Outside Routed Port option of the VPN Service Blade Routed Port Mode Setup Wizard dialog box enables you to use the name and ID of the outside VLAN interface to configure the VLAN configuration port in the routed mode.

## Procedure

1. Right-click on the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard.

2. Click Create. The IPSec VLAN Configuration dialog box appears.

3. Select the radio button Routed Port Mode, then click Configure.... The VPN Service Blade Routed Port Mode Setup Wizard dialog box appears.

4. Select a VLAN from the table or create a new VLAN.

5. Click Next.

The following information appears:

Routed Port

Click Next to view the commands to be sent to the device.

### Routed Port

Name of the routed port.