# CDMA Mobile User Failure Information

The dialog box displays the following information:

> Index (cCdmaFailSessionIndex)

> MS Identifier (cCdmaFailSessionMsid)

> MSID Type (cCdmaFailSessionMsidType)

> Electronic Station Number (cCdmaFailSessionEsn)

> HA IpAddress (cCdmaFailSessionA11HaIp)

> FA IpAddress (cCdmaFailSessionA11FaIp)

> Connection ID (cCdmaFailSessionConnId)

> Session Key (cCdmaFailSessionKey)

> Failure Date & Time (cCdmaFailHistFailTime)

> Failure Type (cCdmaFailHistFailType)

### Index(cCdmaFailSessionIndex)

An arbitrary integer to uniquely identify the entry. Increases monotonically and then wrap to zero.

### MS Identifier(cCdmaFailSessionMsid)

MSID of the mobile station for the failed session.

### MSID Type(cCdmaFailSessionMsidType)

MSID format type of a mobile station for the failed session.

### Electronic Station Number(cCdmaFailSessionEsn)

Electronic station number of the mobile user for the failed session.

### HA IpAddress(cCdmaFailSessionA11HaIp)

Mobile IP home agent address on the A11 interface for the failed session.

### FA IpAddress(cCdmaFailSessionA11FaIp)

Mobile IP foreign agent address on the A11 interface for the failed session.

### Connection ID(cCdmaFailSessionConnId)

Connection ID of the failed session.

### Session Key(cCdmaFailSessionKey)

GRE session identification key of the failed session.

### Failure Date & Time(cCdmaFailHistFailTime)

Date and time of the failure.

### Failure Type(cCdmaFailHistFailType)

Type of failure for the current record.

Possible values are:

Other (1) |
pppAuthenticationFailure (2) |
mobileIPAuthenticaitonFailure (3) |
mobileIPRegistrationTimeout (4) |
a10a11SessionTimeout (5) |
maxAllowedSessionReached (6) |
maxAllowedPcfReached (7) |
sessionFormatError (8) |