# GGSN QOS Mapping

The GGSN QOS Mapping dialog box lists the active PDP contexts that have cggsnQosClass.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN QOS Mapping from the Category list.

3. Select a row in the table and click the Monitor button.

The following information appears:

PDP Contexts Count (cggsnQosCurrentPdps)

### PDP Contexts Count (cggsnQosCurrentPdps)

Number of PDP contexts that have this QOS class.