# Virtual Client Info

To access the Virtual Client Info dialog box:

1. Select Device > Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click Virtual Servers.

3. With an entry selected, click VirClient.

This dialog box provides information regarding the client IP address, client mask, and the range of IP addresses of the clients.

The Virtual Client Info dialog box displays the following information:

- Client IP Address (slbVirtualClientIpAddress)

- Client Mask (slbVirtualClientMask)

- Client Range Exclude (slbVirtualClientExclude)

- Virtual Client Row status (slbVirtualClientRowStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Client IP Address (slbVirtualClientIpAddress)

The IP address of the client. It is used along with the slbVirtualClientMask to represent subsets of client traffic being handled by the virtual server.

Client Mask (slbVirtualClientMask)

The general purpose mask of the client. It is used along with the slbVirtualClientIpAddress to represent subsets of client traffic being handled by the particular virtual server.

Client Range Exclude (slbVirtualClientExclude)

The truth value that determines whether client range should be included or excluded on the virtual server.

Virtual Client Row status (slbVirtualClientRowStatus)

The management station uses row status to create or delete the row entry in slbVirtualClientTable following the RowStatus textual convention.