# Displaying Power Supply Information

To display configuration information for a Catalyst 4000, 5000, 5500, or 6000 power supply, right-click the power supply and select Configure.

The following information is displayed:

Power Supply Type (chassisPsType)

Type of power supply in the chassis.

PS Status (chassisPsStatus)

Status of the power supply. Possible values include OK, minor, major, and other.

- Minor fault or the number 3 indicates a minor problem with the power supply.

- Major fault or the number 4 indicates a major problem with the power supply.

- Other indicates that the status is none of the above.

PS Diagnostic Errors (chassisPsTestResult)

Test result for this power supply. A zero indicates that the supply passed all tests. Bits set in the result indicate error conditions.

Redundant Supply Status (ciscoEnvMonSupplySource)

Indicates whether this power supply is an internal redundant power supply.

PS Fan Status (ciscoEnvMonFanState)

Indicates the status of the power supply fan.

Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.