# SSG Port Maps

This dialog box displays details on the Service Selection Gateway (SSG) port map.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Port Maps from the Category list.

The following information is displayed:

> Port Map Address Type (cssgPortMapSourceIpType)

> Port Map Address (cssgPortMapSourceIp)

> Lower Port Range (cssgPortMapPortRangeFrom)

> Upper Port Range (cssgPortMapPortRangeTo)

> Port Map RowStatus (cssgPortMapRowStatus)

### Port Map Address Type (cssgPortMapSourceIpType)

Value that represents the type of IP address stored in cssgPortMapSourceIP object.

### Port Map Address (cssgPortMapSourceIp)

SSG source IP addresses to be used while translating the network addresses of downstream traffic (traffic from subscriber to SSG).

### Lower Port Range (cssgPortMapPortRangeFrom)

Lower limit of the range of ports in port map.

### Upper Port Range (cssgPortMapPortRangeTo)

Upper limit of the range of ports in port map.

### Port Map RowStatus (cssgPortMapRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo. cssgPortMapPortRangeFrom and cssgPortMapPortRangeTo are mandatory objects for a create request.

- To delete a row, set the object to destroy.