# EOU Details

## Navigation

Device > Configure > EOU > EOU Details

The following information appears:

> Version (cnnEouVersion)

> Posture Validation (cnnEouEnabled)

> Clientless Authentication (cnnEouAllowClientless)

> IP StationID Allowed (cnnEouAllowIpStationId)

> Logging (cnnEouLoggingEnabled)

> Max Retry (cnnEouMaxRetry)

> PortNo (cnnEouPort)

> AAA Timeout (cnnEouTimeoutAAA)

> Hold Period Timout (cnnEouTimeoutHoldPeriod)

> Retransmit Timeout (cnnEouTimeoutRetransmit)

> Revalidation Timeout (cnnEouTimeoutRevalidation)

> Status Query Timeout (cnnEouTimeoutStatusQuery)

### Version (cnnEouVersion)

EOU version in use on the local system. The value zero indicates the current version cannot be determined.

### Posture Validation (cnnEouEnabled)

Indicates whether EOU posture validation is globally enabled on the device.

### Clientless Authentication (cnnEouAllowClientless)

Indicates whether the authentication of clientless hosts is allowed on any system that does not run Cisco Trust Agent.

### IP StationID Allowed (cnnEouAllowIpStationId)

Indicates whether the host IP address is sent in the calling station ID field of a RADIUS server request.

### Logging (cnnEouLoggingEnabled)

Indicates whether EOU system logging events are enabled. Set this object to true to enable Syslog messages at an informational level (Syslog level 6).

### Max Retry (cnnEouMaxRetry)

Maximum number of retry attempts for EOU.

### PortNo (cnnEouPort)

UDP port number used for EOU.

Note: Make sure that this port does not conflict with any other UDP applications.

### AAA Timeout (cnnEouTimeoutAAA)

Timeout period used by a Network Access Device (NAD) with authentication, authorization, and accounting (AAA) enabled.

### Hold Period Timout (cnnEouTimeoutHoldPeriod)

Length of time that elapses before client sessions are purged from the system due to client inactivity.

### Retransmit Timeout (cnnEouTimeoutRetransmit)

Timeout period for a retransmitted EOU message.

### Revalidation Timeout (cnnEouTimeoutRevalidation)

Timeout period for revalidation. Setting this object to zero globally disables periodic revalidation on this device.

### Status Query Timeout (cnnEouTimeoutStatusQuery)

Timeout period for the status query after revalidation.