# Priority Table

Device > Configure > AAA Configuration

This category provides information on entries for AAA authentication methods.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Session (cacSession)

- Authentication (cacAuthen)

- Login Mode (cacLoginMode)

- Method (cacEnable)

- Priority Number (cacPriorityNumber)

- Primary Method (cacPrimaryMethod)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to make changes take effect.

- Click Cancel to close the dialog box.

- Click Refresh to reload the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Session (cacSession)

Session type used to connect to the network device.

Authentication (cacAuthen)

Authentication method to authenticate users.

Login Mode (cacLoginMode)

Mode used to login to the network device.

Method (cacEnable)

Indicates whether the authentication method denoted by cacAuthen is enabled or not.

Priority Number (cacPriorityNumber)

Number used to authenticate a user session.

Primary Method (cacPrimaryMethod)

Indicates whether the authentication method denoted by cacAuthen is the primary (first one to be tried) method when there are multiple authentication methods configured.

Note: You cannot set the current primary method to "false" directly. Instead, you must specify another method as the new primary method.